
\chapter{CFD Wind Loads}
\label{cfd-wind-loads}

\section{30 zenith - 0 azimuth - Open vents/Stowed wind screen - 2m/s}
\label{zen30az000_OS2}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/scenes/vort_tel_vort_tel_9.998000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 32.339 & 20.105 & 0.696 & 123.047 \\
 CringR & 35.165 & 24.994 & 1.226 & 142.592 \\
 Cring strB & 2.370 & 1.379 & 0.089 & 7.669 \\
 Cring strF & 2.796 & 1.678 & 0.079 & 9.581 \\
 Cring strL & 2.261 & 1.652 & 0.026 & 9.065 \\
 Cring strR & 3.001 & 2.201 & 0.019 & 12.289 \\
 GIR & 37.455 & 22.475 & 0.483 & 142.525 \\
 LGSS1 & 3.739 & 2.649 & 0.077 & 15.111 \\
 LGSS2 & 3.713 & 2.561 & 0.092 & 13.714 \\
 LGSS3 & 3.834 & 2.505 & 0.057 & 14.228 \\
 LGSSc & 1.122 & 0.831 & 0.007 & 4.558 \\
 M1Baffle & 16.924 & 12.097 & 0.282 & 64.991 \\
 M1cell & 1025.942 & 725.898 & 8.719 & 3898.329 \\
 M1cov1 & 5.636 & 3.879 & 0.094 & 19.042 \\
 M1cov2 & 3.537 & 2.529 & 0.070 & 16.397 \\
 M1cov3 & 2.326 & 1.670 & 0.032 & 9.514 \\
 M1cov4 & 1.434 & 0.759 & 0.036 & 4.467 \\
 M1cov5 & 2.600 & 1.750 & 0.065 & 9.344 \\
 M1cov6 & 3.155 & 2.190 & 0.042 & 14.269 \\
 M1covin1 & 0.946 & 0.530 & 0.033 & 3.253 \\
 M1covin2 & 0.583 & 0.316 & 0.013 & 2.066 \\
 M1covin3 & 0.652 & 0.357 & 0.021 & 2.399 \\
 M1covin4 & 0.784 & 0.437 & 0.012 & 2.492 \\
 M1covin5 & 0.730 & 0.393 & 0.015 & 2.506 \\
 M1covin6 & 1.070 & 0.567 & 0.042 & 3.617 \\
 M1level & 2.803 & 1.543 & 0.083 & 8.837 \\
 M2Baffle & 0.176 & 0.134 & 0.002 & 0.772 \\
 M2seg1 & 0.092 & 0.042 & 0.002 & 0.279 \\
 M2seg2 & 0.104 & 0.049 & 0.004 & 0.315 \\
 M2seg3 & 0.117 & 0.056 & 0.003 & 0.320 \\
 M2seg4 & 0.078 & 0.034 & 0.003 & 0.279 \\
 M2seg5 & 0.093 & 0.039 & 0.005 & 0.239 \\
 M2seg6 & 0.131 & 0.060 & 0.004 & 0.452 \\
 M2seg7 & 0.164 & 0.100 & 0.005 & 0.590 \\
 Tbot1 & 1.283 & 0.629 & 0.046 & 3.492 \\
 Tbot2 & 2.046 & 0.923 & 0.075 & 5.834 \\
 Tbot3 & 1.788 & 0.985 & 0.024 & 7.555 \\
 Topend & 1.032 & 0.559 & 0.035 & 3.526 \\
 Tup1 & 1.463 & 0.768 & 0.028 & 5.166 \\
 Tup2 & 1.048 & 0.481 & 0.054 & 2.767 \\
 Tup3 & 1.231 & 0.604 & 0.064 & 3.605 \\
 arm1 & 0.372 & 0.217 & 0.005 & 1.194 \\
 arm2 & 0.303 & 0.189 & 0.006 & 1.161 \\
 arm3 & 0.239 & 0.132 & 0.002 & 0.820 \\
 cabletrays & 69.727 & 46.169 & 1.859 & 246.784 \\
 cabletruss & 1.272 & 0.735 & 0.020 & 4.738 \\
 platform & 76.860 & 54.023 & 1.787 & 295.416 \\
 S1 & 10346.765 & 823.066 & 8943.360 & 12296.780 \\
 S2 & 10332.704 & 823.057 & 8925.615 & 12306.434 \\
 S3 & 10335.588 & 822.618 & 8935.404 & 12310.306 \\
 S4 & 10339.074 & 822.471 & 8955.294 & 12297.759 \\
 S5 & 10341.440 & 822.569 & 8935.069 & 12277.234 \\
 S6 & 10340.574 & 822.861 & 8924.366 & 12277.069 \\
 S7 & 8777.561 & 698.052 & 7600.546 & 10429.674 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 2430.985 & 193.196 & 2103.863 & 2890.482 \\
 S2 & 2427.308 & 193.379 & 2083.821 & 2892.887 \\
 S3 & 2427.587 & 193.439 & 2082.561 & 2891.844 \\
 S4 & 2429.318 & 193.459 & 2098.013 & 2887.921 \\
 S5 & 2431.109 & 193.956 & 2089.360 & 2906.804 \\
 S6 & 2431.148 & 193.732 & 2093.188 & 2907.630 \\
 S7 & 1437.636 & 115.344 & 1230.081 & 1724.449 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS2/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 213.061 & 105.080 & 6.986 & 610.922 \\
 CringR & 147.756 & 98.395 & 4.562 & 604.194 \\
 Cring strB & 18.344 & 12.266 & 0.458 & 70.072 \\
 Cring strF & 18.601 & 12.007 & 0.372 & 62.166 \\
 Cring strL & 15.455 & 11.271 & 0.222 & 60.931 \\
 Cring strR & 14.635 & 10.734 & 0.088 & 58.636 \\
 GIR & 131.734 & 83.127 & 2.737 & 506.827 \\
 LGSS1 & 37.641 & 28.482 & 0.379 & 153.418 \\
 LGSS2 & 38.848 & 27.767 & 0.250 & 142.288 \\
 LGSS3 & 39.511 & 28.232 & 0.099 & 146.675 \\
 LGSSc & 10.796 & 7.995 & 0.032 & 43.826 \\
 M1Baffle & 9.021 & 5.275 & 0.121 & 34.507 \\
 M1cell & 1461.849 & 916.306 & 15.929 & 5787.483 \\
 M1cov1 & 64.422 & 42.417 & 1.723 & 209.034 \\
 M1cov2 & 39.255 & 27.782 & 0.472 & 181.037 \\
 M1cov3 & 26.036 & 18.472 & 0.524 & 107.868 \\
 M1cov4 & 17.993 & 9.309 & 0.250 & 57.604 \\
 M1cov5 & 28.372 & 18.750 & 0.444 & 101.703 \\
 M1cov6 & 34.824 & 23.912 & 0.227 & 155.540 \\
 M1covin1 & 6.056 & 3.455 & 0.080 & 21.507 \\
 M1covin2 & 3.807 & 2.127 & 0.066 & 12.454 \\
 M1covin3 & 4.504 & 2.597 & 0.052 & 18.100 \\
 M1covin4 & 5.470 & 3.177 & 0.029 & 17.376 \\
 M1covin5 & 4.736 & 2.608 & 0.033 & 16.112 \\
 M1covin6 & 7.001 & 3.932 & 0.182 & 23.466 \\
 M1level & 27.250 & 14.266 & 1.461 & 81.823 \\
 M2Baffle & 0.335 & 0.184 & 0.005 & 1.317 \\
 M2seg1 & 1.458 & 0.777 & 0.022 & 4.940 \\
 M2seg2 & 1.856 & 0.924 & 0.016 & 5.856 \\
 M2seg3 & 1.660 & 0.871 & 0.019 & 5.758 \\
 M2seg4 & 1.342 & 0.715 & 0.020 & 4.161 \\
 M2seg5 & 1.714 & 0.864 & 0.019 & 5.326 \\
 M2seg6 & 2.303 & 1.316 & 0.037 & 9.108 \\
 M2seg7 & 1.036 & 0.543 & 0.006 & 3.157 \\
 Tbot1 & 12.417 & 7.685 & 0.406 & 45.386 \\
 Tbot2 & 17.932 & 10.772 & 0.398 & 67.155 \\
 Tbot3 & 19.611 & 12.260 & 0.436 & 93.086 \\
 Topend & 12.374 & 6.591 & 0.364 & 41.635 \\
 Tup1 & 23.848 & 12.365 & 0.719 & 85.289 \\
 Tup2 & 16.954 & 8.373 & 0.489 & 51.607 \\
 Tup3 & 19.941 & 10.639 & 0.499 & 60.518 \\
 arm1 & 7.940 & 4.855 & 0.095 & 25.728 \\
 arm2 & 6.513 & 4.214 & 0.095 & 25.455 \\
 arm3 & 4.937 & 2.951 & 0.043 & 17.852 \\
 cabletrays & 158.365 & 112.964 & 3.386 & 648.218 \\
 cabletruss & 20.217 & 12.237 & 0.473 & 70.443 \\
 platform & 94.097 & 46.177 & 2.799 & 307.671 \\
 S1 & 101005.378 & 8036.494 & 87307.282 & 120044.067 \\
 S2 & 100670.269 & 8020.055 & 86947.806 & 119922.960 \\
 S3 & 100705.029 & 8014.575 & 87053.323 & 119967.305 \\
 S4 & 524628.507 & 43309.093 & 438957.642 & 631923.589 \\
 S5 & 100764.850 & 8015.482 & 87046.683 & 119649.230 \\
 S6 & 100734.294 & 8017.830 & 86919.174 & 119624.856 \\
 S7 & 8663.817 & 687.466 & 7494.972 & 10278.644 \\
\bottomrule
\end{longtable}




\section{30 zenith - 45 azimuth - Open vents/Stowed wind screen - 2m/s}
\label{zen30az045_OS2}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/scenes/vort_tel_vort_tel_9.998000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 25.386 & 15.361 & 0.911 & 122.224 \\
 CringR & 30.128 & 20.203 & 0.288 & 119.086 \\
 Cring strB & 2.106 & 1.318 & 0.040 & 8.312 \\
 Cring strF & 2.438 & 1.365 & 0.080 & 6.710 \\
 Cring strL & 1.879 & 1.332 & 0.033 & 6.628 \\
 Cring strR & 2.336 & 1.728 & 0.023 & 7.596 \\
 GIR & 34.809 & 22.103 & 0.751 & 158.085 \\
 LGSS1 & 2.876 & 2.098 & 0.060 & 10.052 \\
 LGSS2 & 2.931 & 2.069 & 0.105 & 9.386 \\
 LGSS3 & 3.045 & 2.056 & 0.056 & 9.765 \\
 LGSSc & 0.857 & 0.647 & 0.009 & 2.796 \\
 M1Baffle & 13.082 & 9.701 & 0.285 & 42.914 \\
 M1cell & 803.291 & 586.794 & 3.746 & 2606.254 \\
 M1cov1 & 3.076 & 2.217 & 0.026 & 14.633 \\
 M1cov2 & 2.366 & 1.723 & 0.062 & 11.381 \\
 M1cov3 & 2.714 & 2.228 & 0.022 & 16.335 \\
 M1cov4 & 1.067 & 0.524 & 0.058 & 3.295 \\
 M1cov5 & 5.846 & 3.940 & 0.174 & 21.424 \\
 M1cov6 & 4.958 & 3.658 & 0.020 & 22.207 \\
 M1covin1 & 0.620 & 0.390 & 0.011 & 3.054 \\
 M1covin2 & 0.525 & 0.354 & 0.008 & 2.490 \\
 M1covin3 & 0.502 & 0.267 & 0.017 & 1.633 \\
 M1covin4 & 0.834 & 0.424 & 0.038 & 2.389 \\
 M1covin5 & 0.925 & 0.507 & 0.040 & 2.880 \\
 M1covin6 & 0.594 & 0.340 & 0.011 & 2.065 \\
 M1level & 3.420 & 2.222 & 0.151 & 17.580 \\
 M2Baffle & 0.148 & 0.127 & 0.001 & 1.078 \\
 M2seg1 & 0.067 & 0.043 & 0.003 & 0.326 \\
 M2seg2 & 0.064 & 0.045 & 0.002 & 0.372 \\
 M2seg3 & 0.070 & 0.041 & 0.002 & 0.249 \\
 M2seg4 & 0.065 & 0.036 & 0.002 & 0.296 \\
 M2seg5 & 0.063 & 0.037 & 0.003 & 0.325 \\
 M2seg6 & 0.067 & 0.041 & 0.002 & 0.325 \\
 M2seg7 & 0.123 & 0.091 & 0.001 & 0.455 \\
 Tbot1 & 0.953 & 0.512 & 0.052 & 3.391 \\
 Tbot2 & 1.028 & 0.619 & 0.038 & 3.763 \\
 Tbot3 & 1.207 & 0.738 & 0.044 & 5.011 \\
 Topend & 0.841 & 0.444 & 0.048 & 2.483 \\
 Tup1 & 0.985 & 0.704 & 0.020 & 4.391 \\
 Tup2 & 0.664 & 0.431 & 0.031 & 3.309 \\
 Tup3 & 1.045 & 0.565 & 0.026 & 3.676 \\
 arm1 & 0.208 & 0.174 & 0.006 & 1.518 \\
 arm2 & 0.231 & 0.194 & 0.005 & 1.160 \\
 arm3 & 0.383 & 0.228 & 0.017 & 1.427 \\
 cabletrays & 55.968 & 38.103 & 0.869 & 182.138 \\
 cabletruss & 1.132 & 0.648 & 0.034 & 4.008 \\
 platform & 61.310 & 41.939 & 0.894 & 195.597 \\
 S1 & 24668.772 & 2496.396 & 20632.479 & 29074.443 \\
 S2 & 24672.321 & 2496.345 & 20636.349 & 29120.628 \\
 S3 & 24671.240 & 2496.710 & 20629.207 & 29133.426 \\
 S4 & 24670.140 & 2496.569 & 20641.807 & 29103.190 \\
 S5 & 24658.380 & 2497.518 & 20608.791 & 29081.819 \\
 S6 & 24659.070 & 2497.479 & 20588.642 & 29085.343 \\
 S7 & 20940.740 & 2119.886 & 17528.173 & 24691.165 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 5792.788 & 586.325 & 4842.918 & 6838.219 \\
 S2 & 5792.285 & 586.628 & 4829.564 & 6840.852 \\
 S3 & 5795.725 & 587.096 & 4822.757 & 6850.547 \\
 S4 & 5800.243 & 587.015 & 4845.620 & 6840.982 \\
 S5 & 5799.369 & 586.883 & 4837.538 & 6852.538 \\
 S6 & 5795.888 & 586.614 & 4831.788 & 6858.095 \\
 S7 & 3430.463 & 347.972 & 2818.911 & 4080.255 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS2/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 172.479 & 89.136 & 4.651 & 633.439 \\
 CringR & 145.909 & 100.238 & 2.806 & 648.952 \\
 Cring strB & 14.474 & 9.249 & 0.326 & 43.547 \\
 Cring strF & 15.446 & 10.233 & 0.229 & 58.471 \\
 Cring strL & 12.516 & 9.136 & 0.137 & 41.613 \\
 Cring strR & 11.379 & 8.588 & 0.188 & 36.724 \\
 GIR & 115.885 & 75.686 & 1.174 & 554.073 \\
 LGSS1 & 29.480 & 22.218 & 0.151 & 103.855 \\
 LGSS2 & 31.093 & 22.177 & 0.138 & 101.194 \\
 LGSS3 & 30.677 & 22.589 & 0.082 & 105.504 \\
 LGSSc & 8.199 & 6.215 & 0.031 & 26.685 \\
 M1Baffle & 6.925 & 3.700 & 0.091 & 22.901 \\
 M1cell & 1331.900 & 867.981 & 7.497 & 6342.927 \\
 M1cov1 & 36.374 & 25.268 & 0.324 & 170.061 \\
 M1cov2 & 26.771 & 18.836 & 0.405 & 127.512 \\
 M1cov3 & 29.197 & 24.238 & 0.714 & 185.972 \\
 M1cov4 & 13.543 & 7.492 & 0.117 & 49.083 \\
 M1cov5 & 68.386 & 43.663 & 2.589 & 233.397 \\
 M1cov6 & 55.961 & 41.105 & 0.788 & 245.679 \\
 M1covin1 & 4.101 & 2.612 & 0.069 & 18.378 \\
 M1covin2 & 3.371 & 2.335 & 0.090 & 15.527 \\
 M1covin3 & 3.280 & 1.816 & 0.092 & 10.353 \\
 M1covin4 & 5.427 & 2.930 & 0.068 & 17.516 \\
 M1covin5 & 6.513 & 3.771 & 0.180 & 21.037 \\
 M1covin6 & 4.026 & 2.423 & 0.018 & 14.840 \\
 M1level & 28.908 & 15.391 & 0.660 & 101.425 \\
 M2Baffle & 0.207 & 0.138 & 0.002 & 0.856 \\
 M2seg1 & 0.955 & 0.606 & 0.005 & 3.735 \\
 M2seg2 & 0.902 & 0.607 & 0.018 & 4.682 \\
 M2seg3 & 1.087 & 0.738 & 0.013 & 5.330 \\
 M2seg4 & 0.986 & 0.587 & 0.010 & 3.720 \\
 M2seg5 & 0.954 & 0.552 & 0.006 & 3.417 \\
 M2seg6 & 1.022 & 0.627 & 0.016 & 4.027 \\
 M2seg7 & 0.671 & 0.389 & 0.004 & 2.372 \\
 Tbot1 & 7.732 & 5.319 & 0.268 & 33.220 \\
 Tbot2 & 9.463 & 7.127 & 0.279 & 47.678 \\
 Tbot3 & 11.422 & 8.743 & 0.447 & 63.103 \\
 Topend & 10.310 & 6.296 & 0.278 & 39.951 \\
 Tup1 & 14.420 & 10.263 & 0.215 & 58.031 \\
 Tup2 & 11.009 & 7.479 & 0.283 & 50.869 \\
 Tup3 & 16.324 & 9.072 & 0.565 & 56.335 \\
 arm1 & 4.434 & 3.846 & 0.073 & 33.145 \\
 arm2 & 4.970 & 4.317 & 0.026 & 25.621 \\
 arm3 & 8.194 & 5.131 & 0.106 & 31.413 \\
 cabletrays & 133.407 & 92.791 & 3.308 & 530.793 \\
 cabletruss & 17.217 & 10.083 & 0.501 & 61.375 \\
 platform & 63.641 & 34.384 & 2.856 & 260.661 \\
 S1 & 240376.721 & 24328.617 & 201035.706 & 283310.219 \\
 S2 & 240372.778 & 24323.321 & 201035.168 & 283721.129 \\
 S3 & 240361.122 & 24324.567 & 200959.708 & 283844.879 \\
 S4 & 240363.732 & 24323.412 & 201103.033 & 283562.137 \\
 S5 & 240254.037 & 24336.955 & 200796.173 & 283363.300 \\
 S6 & 240269.112 & 24333.627 & 200582.680 & 283418.353 \\
 S7 & 1516.509 & 151.938 & 1269.257 & 1798.176 \\
\bottomrule
\end{longtable}




\section{30 zenith - 90 azimuth - Open vents/Stowed wind screen - 2m/s}
\label{zen30az090_OS2}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/scenes/vort_tel_vort_tel_9.998000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 4.257 & 2.044 & 0.290 & 10.763 \\
 CringR & 1.910 & 1.245 & 0.055 & 6.141 \\
 Cring strB & 0.228 & 0.132 & 0.006 & 0.839 \\
 Cring strF & 0.282 & 0.165 & 0.007 & 1.051 \\
 Cring strL & 0.557 & 0.256 & 0.020 & 1.486 \\
 Cring strR & 0.258 & 0.192 & 0.008 & 0.982 \\
 GIR & 2.096 & 1.038 & 0.093 & 6.683 \\
 LGSS1 & 0.540 & 0.288 & 0.003 & 1.552 \\
 LGSS2 & 0.772 & 0.329 & 0.049 & 1.919 \\
 LGSS3 & 0.516 & 0.288 & 0.008 & 1.630 \\
 LGSSc & 0.093 & 0.072 & 0.005 & 0.358 \\
 M1Baffle & 1.660 & 0.986 & 0.032 & 5.084 \\
 M1cell & 87.345 & 65.080 & 0.931 & 317.975 \\
 M1cov1 & 0.981 & 0.672 & 0.046 & 3.751 \\
 M1cov2 & 0.742 & 0.526 & 0.023 & 3.291 \\
 M1cov3 & 0.794 & 0.545 & 0.016 & 2.570 \\
 M1cov4 & 1.213 & 0.922 & 0.017 & 5.489 \\
 M1cov5 & 3.216 & 2.192 & 0.023 & 14.586 \\
 M1cov6 & 1.549 & 1.015 & 0.058 & 5.739 \\
 M1covin1 & 0.464 & 0.270 & 0.006 & 1.947 \\
 M1covin2 & 0.355 & 0.199 & 0.007 & 1.382 \\
 M1covin3 & 0.400 & 0.226 & 0.022 & 1.243 \\
 M1covin4 & 0.706 & 0.358 & 0.017 & 2.175 \\
 M1covin5 & 0.713 & 0.409 & 0.020 & 2.776 \\
 M1covin6 & 0.738 & 0.397 & 0.021 & 2.836 \\
 M1level & 2.284 & 1.342 & 0.046 & 7.556 \\
 M2Baffle & 0.131 & 0.114 & 0.001 & 0.683 \\
 M2seg1 & 0.042 & 0.029 & 0.002 & 0.182 \\
 M2seg2 & 0.042 & 0.028 & 0.004 & 0.169 \\
 M2seg3 & 0.053 & 0.033 & 0.002 & 0.246 \\
 M2seg4 & 0.046 & 0.027 & 0.003 & 0.150 \\
 M2seg5 & 0.041 & 0.029 & 0.001 & 0.220 \\
 M2seg6 & 0.040 & 0.029 & 0.002 & 0.199 \\
 M2seg7 & 0.040 & 0.030 & 0.002 & 0.173 \\
 Tbot1 & 0.488 & 0.288 & 0.008 & 1.784 \\
 Tbot2 & 0.546 & 0.314 & 0.017 & 1.668 \\
 Tbot3 & 1.022 & 0.634 & 0.028 & 3.989 \\
 Topend & 0.197 & 0.094 & 0.005 & 0.600 \\
 Tup1 & 0.502 & 0.426 & 0.006 & 3.193 \\
 Tup2 & 0.337 & 0.205 & 0.026 & 1.573 \\
 Tup3 & 1.013 & 0.622 & 0.019 & 3.985 \\
 arm1 & 0.121 & 0.090 & 0.007 & 0.466 \\
 arm2 & 0.100 & 0.054 & 0.003 & 0.290 \\
 arm3 & 0.370 & 0.214 & 0.009 & 1.416 \\
 cabletrays & 6.725 & 4.387 & 0.185 & 24.716 \\
 cabletruss & 0.863 & 0.495 & 0.029 & 3.245 \\
 platform & 7.909 & 4.955 & 0.382 & 26.951 \\
 S1 & 3860.292 & 17.140 & 3809.138 & 3903.212 \\
 S2 & 3860.950 & 17.228 & 3808.783 & 3899.886 \\
 S3 & 3855.120 & 17.438 & 3800.970 & 3894.471 \\
 S4 & 3852.302 & 16.971 & 3800.041 & 3893.354 \\
 S5 & 3854.293 & 16.424 & 3804.572 & 3893.962 \\
 S6 & 3856.870 & 17.174 & 3802.466 & 3897.469 \\
 S7 & 3271.954 & 14.349 & 3227.473 & 3307.240 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 906.001 & 3.984 & 894.355 & 915.371 \\
 S2 & 908.369 & 3.973 & 896.745 & 917.514 \\
 S3 & 909.201 & 4.062 & 897.016 & 918.953 \\
 S4 & 908.259 & 4.060 & 895.804 & 918.215 \\
 S5 & 906.301 & 4.039 & 893.989 & 915.988 \\
 S6 & 904.949 & 4.084 & 892.252 & 914.743 \\
 S7 & 551.451 & 3.155 & 541.905 & 558.344 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS2/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 30.302 & 15.549 & 0.308 & 94.814 \\
 CringR & 7.477 & 3.479 & 0.666 & 20.421 \\
 Cring strB & 1.877 & 1.041 & 0.098 & 5.982 \\
 Cring strF & 1.805 & 1.061 & 0.050 & 5.445 \\
 Cring strL & 4.256 & 2.204 & 0.115 & 18.101 \\
 Cring strR & 1.379 & 0.938 & 0.076 & 4.939 \\
 GIR & 6.415 & 2.861 & 0.316 & 24.229 \\
 LGSS1 & 4.386 & 3.232 & 0.021 & 16.785 \\
 LGSS2 & 6.186 & 3.155 & 0.153 & 17.213 \\
 LGSS3 & 4.999 & 3.401 & 0.031 & 17.074 \\
 LGSSc & 0.877 & 0.685 & 0.002 & 3.461 \\
 M1Baffle & 2.888 & 1.824 & 0.028 & 11.395 \\
 M1cell & 79.001 & 38.901 & 10.607 & 195.935 \\
 M1cov1 & 11.508 & 7.590 & 0.437 & 42.684 \\
 M1cov2 & 7.818 & 5.505 & 0.322 & 32.702 \\
 M1cov3 & 8.818 & 5.678 & 0.438 & 28.126 \\
 M1cov4 & 14.095 & 10.838 & 0.259 & 64.821 \\
 M1cov5 & 38.867 & 27.089 & 0.951 & 187.448 \\
 M1cov6 & 17.562 & 10.525 & 1.255 & 59.953 \\
 M1covin1 & 2.945 & 1.686 & 0.136 & 12.896 \\
 M1covin2 & 2.259 & 1.304 & 0.032 & 9.287 \\
 M1covin3 & 2.498 & 1.422 & 0.075 & 8.251 \\
 M1covin4 & 4.512 & 2.415 & 0.074 & 16.038 \\
 M1covin5 & 4.866 & 2.908 & 0.168 & 20.667 \\
 M1covin6 & 4.536 & 2.460 & 0.089 & 15.844 \\
 M1level & 28.457 & 14.108 & 1.796 & 84.220 \\
 M2Baffle & 0.156 & 0.106 & 0.003 & 0.851 \\
 M2seg1 & 0.458 & 0.321 & 0.014 & 1.974 \\
 M2seg2 & 0.455 & 0.275 & 0.002 & 1.732 \\
 M2seg3 & 0.733 & 0.539 & 0.021 & 5.732 \\
 M2seg4 & 0.560 & 0.320 & 0.005 & 2.474 \\
 M2seg5 & 0.444 & 0.260 & 0.004 & 1.822 \\
 M2seg6 & 0.445 & 0.270 & 0.003 & 1.651 \\
 M2seg7 & 0.269 & 0.173 & 0.002 & 0.943 \\
 Tbot1 & 5.048 & 3.339 & 0.135 & 20.790 \\
 Tbot2 & 5.130 & 3.399 & 0.309 & 18.483 \\
 Tbot3 & 11.933 & 8.124 & 0.654 & 52.730 \\
 Topend & 3.978 & 2.292 & 0.112 & 14.058 \\
 Tup1 & 7.317 & 6.013 & 0.242 & 42.924 \\
 Tup2 & 5.076 & 2.910 & 0.163 & 18.405 \\
 Tup3 & 15.938 & 9.251 & 0.423 & 54.477 \\
 arm1 & 2.549 & 1.987 & 0.027 & 10.045 \\
 arm2 & 2.105 & 1.245 & 0.011 & 6.331 \\
 arm3 & 7.908 & 4.720 & 0.175 & 30.363 \\
 cabletrays & 34.283 & 15.319 & 1.997 & 101.238 \\
 cabletruss & 13.192 & 7.795 & 0.229 & 54.066 \\
 platform & 51.973 & 23.834 & 3.307 & 132.183 \\
 S1 & 37608.300 & 168.213 & 37107.061 & 38027.600 \\
 S2 & 37610.690 & 168.061 & 37098.746 & 37993.470 \\
 S3 & 37552.747 & 168.521 & 37032.151 & 37929.451 \\
 S4 & 37533.657 & 165.633 & 37020.091 & 37934.894 \\
 S5 & 37564.251 & 159.981 & 37080.923 & 37950.117 \\
 S6 & 37586.044 & 167.601 & 37056.447 & 37982.369 \\
 S7 & 526.148 & 3.200 & 516.168 & 533.726 \\
\bottomrule
\end{longtable}




\section{30 zenith - 0 azimuth - Open vents/Stowed wind screen - 7m/s}
\label{zen30az000_OS7}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/scenes/vort_tel_vort_tel_7.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 33.783 & 19.580 & 0.852 & 130.204 \\
 CringR & 36.353 & 24.708 & 0.904 & 146.987 \\
 Cring strB & 5.989 & 3.101 & 0.123 & 21.472 \\
 Cring strF & 4.973 & 2.687 & 0.277 & 17.031 \\
 Cring strL & 2.614 & 2.075 & 0.034 & 12.548 \\
 Cring strR & 3.312 & 2.873 & 0.045 & 15.806 \\
 GIR & 42.512 & 19.222 & 2.095 & 115.004 \\
 LGSS1 & 4.178 & 3.430 & 0.117 & 19.134 \\
 LGSS2 & 5.139 & 3.537 & 0.145 & 26.240 \\
 LGSS3 & 8.902 & 5.114 & 0.183 & 33.490 \\
 LGSSc & 1.172 & 1.083 & 0.045 & 6.010 \\
 M1Baffle & 24.508 & 16.066 & 0.918 & 94.027 \\
 M1cell & 1033.868 & 1022.444 & 8.677 & 5554.287 \\
 M1cov1 & 46.937 & 32.010 & 0.853 & 182.376 \\
 M1cov2 & 8.317 & 6.044 & 0.102 & 42.251 \\
 M1cov3 & 4.384 & 3.234 & 0.114 & 18.263 \\
 M1cov4 & 10.382 & 8.664 & 0.187 & 64.651 \\
 M1cov5 & 5.624 & 4.304 & 0.074 & 28.128 \\
 M1cov6 & 11.639 & 8.748 & 0.186 & 79.186 \\
 M1covin1 & 7.436 & 4.391 & 0.208 & 35.123 \\
 M1covin2 & 4.170 & 2.728 & 0.031 & 23.448 \\
 M1covin3 & 5.014 & 3.514 & 0.174 & 35.965 \\
 M1covin4 & 7.610 & 4.198 & 0.141 & 28.878 \\
 M1covin5 & 5.355 & 2.885 & 0.295 & 21.387 \\
 M1covin6 & 8.848 & 4.572 & 0.152 & 31.973 \\
 M1level & 9.688 & 6.193 & 0.563 & 53.057 \\
 M2Baffle & 1.760 & 1.292 & 0.009 & 7.750 \\
 M2seg1 & 0.847 & 0.413 & 0.044 & 2.987 \\
 M2seg2 & 0.803 & 0.375 & 0.031 & 2.592 \\
 M2seg3 & 1.350 & 0.713 & 0.053 & 4.745 \\
 M2seg4 & 0.802 & 0.362 & 0.029 & 2.714 \\
 M2seg5 & 1.092 & 0.456 & 0.044 & 3.393 \\
 M2seg6 & 1.474 & 0.686 & 0.028 & 4.745 \\
 M2seg7 & 0.779 & 0.373 & 0.041 & 2.692 \\
 Tbot1 & 11.316 & 6.854 & 0.309 & 51.798 \\
 Tbot2 & 17.493 & 10.321 & 0.741 & 87.405 \\
 Tbot3 & 13.551 & 7.252 & 0.379 & 54.292 \\
 Topend & 3.839 & 1.671 & 0.171 & 12.581 \\
 Tup1 & 13.505 & 7.867 & 0.312 & 52.982 \\
 Tup2 & 7.036 & 3.748 & 0.110 & 34.236 \\
 Tup3 & 10.869 & 5.614 & 0.283 & 48.669 \\
 arm1 & 2.761 & 1.516 & 0.080 & 10.519 \\
 arm2 & 1.792 & 1.125 & 0.041 & 7.253 \\
 arm3 & 2.082 & 1.228 & 0.071 & 8.746 \\
 cabletrays & 72.813 & 66.845 & 1.221 & 389.306 \\
 cabletruss & 9.670 & 5.184 & 0.529 & 35.135 \\
 platform & 78.215 & 71.289 & 2.151 & 395.668 \\
 S1 & 2118.136 & 651.850 & 1109.488 & 3953.412 \\
 S2 & 1926.986 & 644.971 & 885.059 & 3745.356 \\
 S3 & 1910.884 & 646.307 & 854.854 & 3743.152 \\
 S4 & 1926.080 & 653.206 & 860.872 & 3803.325 \\
 S5 & 1918.237 & 647.667 & 861.509 & 3738.711 \\
 S6 & 1970.906 & 649.705 & 875.916 & 3804.206 \\
 S7 & 1693.946 & 556.015 & 786.218 & 3226.439 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 527.056 & 145.786 & 284.013 & 952.245 \\
 S2 & 456.996 & 151.834 & 205.014 & 891.669 \\
 S3 & 453.036 & 152.260 & 192.934 & 887.413 \\
 S4 & 453.443 & 152.721 & 204.440 & 891.211 \\
 S5 & 450.358 & 151.599 & 198.798 & 881.097 \\
 S6 & 463.117 & 151.052 & 202.077 & 897.701 \\
 S7 & 208.214 & 92.664 & 9.340 & 552.747 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_OS7/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 266.360 & 147.673 & 3.329 & 885.417 \\
 CringR & 206.146 & 119.555 & 4.859 & 766.604 \\
 Cring strB & 40.336 & 23.016 & 1.267 & 187.010 \\
 Cring strF & 35.057 & 19.556 & 1.161 & 113.546 \\
 Cring strL & 18.404 & 14.552 & 0.485 & 86.388 \\
 Cring strR & 18.018 & 13.969 & 0.262 & 81.624 \\
 GIR & 128.558 & 69.122 & 2.518 & 412.600 \\
 LGSS1 & 42.900 & 37.056 & 0.366 & 204.513 \\
 LGSS2 & 47.196 & 36.780 & 0.351 & 289.173 \\
 LGSS3 & 58.691 & 40.480 & 1.144 & 271.510 \\
 LGSSc & 10.968 & 10.388 & 0.070 & 56.735 \\
 M1Baffle & 63.933 & 40.621 & 1.190 & 290.222 \\
 M1cell & 1018.724 & 576.810 & 28.706 & 3220.946 \\
 M1cov1 & 517.964 & 353.993 & 5.427 & 1957.584 \\
 M1cov2 & 95.166 & 69.832 & 3.167 & 418.868 \\
 M1cov3 & 48.478 & 35.127 & 0.495 & 205.169 \\
 M1cov4 & 117.565 & 97.155 & 1.554 & 750.753 \\
 M1cov5 & 63.213 & 46.662 & 1.014 & 319.805 \\
 M1cov6 & 128.651 & 96.946 & 3.108 & 883.373 \\
 M1covin1 & 46.735 & 27.773 & 0.569 & 208.319 \\
 M1covin2 & 26.807 & 18.483 & 0.596 & 171.845 \\
 M1covin3 & 31.995 & 23.961 & 0.482 & 267.032 \\
 M1covin4 & 52.553 & 29.948 & 1.033 & 214.941 \\
 M1covin5 & 34.586 & 18.923 & 0.724 & 129.742 \\
 M1covin6 & 56.493 & 30.020 & 1.237 & 218.236 \\
 M1level & 139.798 & 86.998 & 6.172 & 733.614 \\
 M2Baffle & 3.288 & 1.763 & 0.066 & 11.215 \\
 M2seg1 & 12.717 & 6.748 & 0.214 & 44.276 \\
 M2seg2 & 13.472 & 7.293 & 0.149 & 52.163 \\
 M2seg3 & 16.818 & 8.667 & 0.088 & 65.811 \\
 M2seg4 & 12.997 & 6.945 & 0.200 & 44.573 \\
 M2seg5 & 19.717 & 9.756 & 0.189 & 61.919 \\
 M2seg6 & 26.063 & 14.312 & 0.221 & 93.792 \\
 M2seg7 & 11.097 & 5.962 & 0.077 & 42.959 \\
 Tbot1 & 142.323 & 92.574 & 1.605 & 680.390 \\
 Tbot2 & 184.100 & 115.961 & 3.606 & 1017.677 \\
 Tbot3 & 151.319 & 85.879 & 4.332 & 715.482 \\
 Topend & 73.653 & 38.399 & 2.611 & 241.161 \\
 Tup1 & 219.416 & 119.912 & 6.155 & 749.198 \\
 Tup2 & 113.524 & 59.990 & 2.525 & 483.511 \\
 Tup3 & 171.732 & 90.064 & 7.506 & 709.184 \\
 arm1 & 57.623 & 34.106 & 0.901 & 231.556 \\
 arm2 & 38.351 & 25.147 & 0.621 & 159.086 \\
 arm3 & 43.576 & 27.530 & 1.072 & 188.425 \\
 cabletrays & 232.189 & 139.324 & 17.023 & 976.488 \\
 cabletruss & 155.478 & 85.785 & 5.365 & 638.348 \\
 platform & 278.139 & 155.709 & 14.870 & 1095.825 \\
 S1 & 20661.654 & 6341.938 & 10828.092 & 38413.523 \\
 S2 & 18709.476 & 6277.260 & 8570.758 & 36420.090 \\
 S3 & 18602.710 & 6296.323 & 8321.009 & 36475.351 \\
 S4 & 18756.618 & 6367.111 & 8363.080 & 37086.280 \\
 S5 & 18657.505 & 6308.302 & 8337.822 & 36378.547 \\
 S6 & 19124.348 & 6321.014 & 8452.976 & 36986.316 \\
 S7 & 280.116 & 90.922 & 98.562 & 560.817 \\
\bottomrule
\end{longtable}




\section{30 zenith - 45 azimuth - Open vents/Stowed wind screen - 7m/s}
\label{zen30az045_OS7}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/scenes/vort_tel_vort_tel_7.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 23.462 & 11.255 & 0.692 & 76.497 \\
 CringR & 10.697 & 6.441 & 0.451 & 39.741 \\
 Cring strB & 1.755 & 0.836 & 0.064 & 5.388 \\
 Cring strF & 1.345 & 0.638 & 0.062 & 3.705 \\
 Cring strL & 2.924 & 1.574 & 0.133 & 12.116 \\
 Cring strR & 0.681 & 0.384 & 0.021 & 2.197 \\
 GIR & 16.253 & 7.159 & 1.170 & 55.352 \\
 LGSS1 & 2.561 & 1.536 & 0.093 & 11.063 \\
 LGSS2 & 3.120 & 1.538 & 0.068 & 11.402 \\
 LGSS3 & 1.977 & 0.922 & 0.052 & 5.527 \\
 LGSSc & 0.251 & 0.137 & 0.003 & 0.846 \\
 M1Baffle & 8.307 & 4.357 & 0.155 & 35.419 \\
 M1cell & 198.784 & 134.515 & 3.669 & 749.269 \\
 M1cov1 & 5.662 & 3.758 & 0.292 & 22.915 \\
 M1cov2 & 8.961 & 6.624 & 0.142 & 41.800 \\
 M1cov3 & 7.984 & 5.210 & 0.068 & 29.156 \\
 M1cov4 & 4.165 & 2.940 & 0.100 & 21.652 \\
 M1cov5 & 34.604 & 24.387 & 0.427 & 194.487 \\
 M1cov6 & 4.940 & 3.753 & 0.075 & 24.842 \\
 M1covin1 & 1.766 & 1.221 & 0.028 & 8.266 \\
 M1covin2 & 2.915 & 1.748 & 0.109 & 14.326 \\
 M1covin3 & 3.546 & 2.047 & 0.043 & 14.120 \\
 M1covin4 & 6.472 & 3.570 & 0.209 & 26.675 \\
 M1covin5 & 5.438 & 3.704 & 0.262 & 28.668 \\
 M1covin6 & 1.776 & 1.406 & 0.051 & 14.765 \\
 M1level & 9.147 & 4.830 & 0.258 & 31.713 \\
 M2Baffle & 1.862 & 1.500 & 0.005 & 10.113 \\
 M2seg1 & 0.648 & 0.423 & 0.028 & 4.238 \\
 M2seg2 & 0.681 & 0.451 & 0.018 & 4.201 \\
 M2seg3 & 0.824 & 0.530 & 0.020 & 4.699 \\
 M2seg4 & 0.773 & 0.513 & 0.019 & 4.310 \\
 M2seg5 & 0.665 & 0.435 & 0.022 & 3.637 \\
 M2seg6 & 0.621 & 0.417 & 0.019 & 3.210 \\
 M2seg7 & 0.618 & 0.444 & 0.023 & 4.821 \\
 Tbot1 & 4.475 & 2.427 & 0.219 & 18.050 \\
 Tbot2 & 5.894 & 3.432 & 0.250 & 24.138 \\
 Tbot3 & 5.834 & 3.690 & 0.145 & 23.643 \\
 Topend & 3.170 & 1.633 & 0.135 & 12.231 \\
 Tup1 & 6.943 & 5.034 & 0.180 & 51.247 \\
 Tup2 & 3.330 & 2.016 & 0.133 & 14.002 \\
 Tup3 & 11.236 & 6.062 & 0.500 & 43.129 \\
 arm1 & 1.726 & 1.296 & 0.044 & 11.888 \\
 arm2 & 1.715 & 1.364 & 0.043 & 11.222 \\
 arm3 & 3.929 & 2.453 & 0.091 & 18.250 \\
 cabletrays & 18.772 & 9.082 & 1.115 & 75.794 \\
 cabletruss & 9.366 & 5.685 & 0.279 & 35.453 \\
 platform & 27.151 & 15.284 & 0.900 & 98.744 \\
 S1 & 3575.552 & 58.281 & 3425.117 & 3722.933 \\
 S2 & 3609.900 & 58.411 & 3458.510 & 3740.758 \\
 S3 & 3607.784 & 57.386 & 3468.044 & 3748.015 \\
 S4 & 3559.004 & 56.064 & 3414.181 & 3695.144 \\
 S5 & 3496.804 & 58.717 & 3336.079 & 3626.325 \\
 S6 & 3561.857 & 59.441 & 3386.742 & 3713.551 \\
 S7 & 3049.056 & 49.601 & 2919.218 & 3189.659 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 831.612 & 13.601 & 795.515 & 866.995 \\
 S2 & 831.030 & 14.346 & 791.989 & 864.935 \\
 S3 & 840.925 & 14.017 & 804.064 & 875.645 \\
 S4 & 849.407 & 13.377 & 815.375 & 884.153 \\
 S5 & 849.660 & 13.368 & 812.952 & 885.995 \\
 S6 & 846.150 & 13.656 & 809.790 & 886.108 \\
 S7 & 499.714 & 20.524 & 437.552 & 558.974 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_OS7/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 143.897 & 70.601 & 4.008 & 425.866 \\
 CringR & 70.219 & 38.267 & 4.046 & 261.830 \\
 Cring strB & 9.907 & 5.028 & 0.425 & 31.664 \\
 Cring strF & 7.876 & 4.134 & 0.241 & 26.395 \\
 Cring strL & 19.390 & 11.501 & 0.497 & 83.259 \\
 Cring strR & 3.547 & 1.902 & 0.038 & 10.745 \\
 GIR & 48.322 & 26.172 & 1.333 & 186.940 \\
 LGSS1 & 14.644 & 8.522 & 0.153 & 56.611 \\
 LGSS2 & 27.199 & 15.273 & 0.107 & 116.302 \\
 LGSS3 & 17.252 & 9.962 & 0.207 & 61.376 \\
 LGSSc & 2.310 & 1.412 & 0.049 & 9.224 \\
 M1Baffle & 33.607 & 21.428 & 0.133 & 175.893 \\
 M1cell & 519.359 & 270.090 & 26.783 & 1813.561 \\
 M1cov1 & 65.108 & 42.256 & 2.526 & 270.644 \\
 M1cov2 & 94.387 & 70.317 & 2.014 & 431.397 \\
 M1cov3 & 84.906 & 60.540 & 0.878 & 337.176 \\
 M1cov4 & 47.136 & 32.082 & 1.143 & 224.763 \\
 M1cov5 & 421.101 & 288.558 & 11.582 & 2390.964 \\
 M1cov6 & 56.397 & 40.835 & 1.390 & 256.270 \\
 M1covin1 & 11.574 & 8.225 & 0.237 & 53.108 \\
 M1covin2 & 18.283 & 10.968 & 0.863 & 80.637 \\
 M1covin3 & 22.213 & 12.788 & 0.594 & 86.894 \\
 M1covin4 & 40.733 & 22.990 & 1.455 & 192.912 \\
 M1covin5 & 37.791 & 27.150 & 0.616 & 215.866 \\
 M1covin6 & 12.266 & 9.942 & 0.254 & 108.522 \\
 M1level & 123.759 & 66.287 & 1.114 & 544.826 \\
 M2Baffle & 2.328 & 1.545 & 0.021 & 12.326 \\
 M2seg1 & 8.183 & 5.218 & 0.112 & 35.929 \\
 M2seg2 & 8.458 & 5.444 & 0.024 & 40.904 \\
 M2seg3 & 11.188 & 7.629 & 0.163 & 51.659 \\
 M2seg4 & 9.689 & 6.079 & 0.056 & 39.164 \\
 M2seg5 & 8.041 & 5.309 & 0.074 & 42.010 \\
 M2seg6 & 7.493 & 4.684 & 0.055 & 38.437 \\
 M2seg7 & 5.521 & 3.756 & 0.079 & 25.690 \\
 Tbot1 & 47.148 & 28.627 & 0.858 & 228.871 \\
 Tbot2 & 63.792 & 42.025 & 2.051 & 298.652 \\
 Tbot3 & 77.621 & 50.964 & 1.309 & 315.482 \\
 Topend & 69.977 & 40.305 & 0.988 & 295.040 \\
 Tup1 & 107.131 & 71.069 & 3.715 & 658.593 \\
 Tup2 & 54.833 & 33.053 & 0.734 & 227.372 \\
 Tup3 & 174.005 & 92.850 & 3.780 & 596.181 \\
 arm1 & 36.629 & 28.720 & 0.226 & 262.781 \\
 arm2 & 36.591 & 30.424 & 0.468 & 249.815 \\
 arm3 & 83.002 & 54.755 & 1.108 & 402.913 \\
 cabletrays & 134.000 & 65.626 & 3.293 & 446.564 \\
 cabletruss & 152.833 & 97.235 & 6.201 & 616.045 \\
 platform & 277.232 & 147.241 & 5.594 & 981.871 \\
 S1 & 34826.722 & 566.177 & 33382.539 & 36264.785 \\
 S2 & 35163.263 & 570.498 & 33670.479 & 36435.318 \\
 S3 & 35125.799 & 561.034 & 33755.746 & 36506.045 \\
 S4 & 34655.277 & 546.917 & 33228.906 & 35953.223 \\
 S5 & 33986.268 & 576.329 & 32400.328 & 35226.869 \\
 S6 & 34680.742 & 577.911 & 32994.506 & 36130.575 \\
 S7 & 220.901 & 24.025 & 92.949 & 296.144 \\
\bottomrule
\end{longtable}




\section{30 zenith - 90 azimuth - Open vents/Stowed wind screen - 7m/s}
\label{zen30az090_OS7}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/scenes/vort_tel_vort_tel_7.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 53.362 & 25.917 & 3.009 & 179.441 \\
 CringR & 16.170 & 8.972 & 0.876 & 43.696 \\
 Cring strB & 2.698 & 1.292 & 0.065 & 8.705 \\
 Cring strF & 2.186 & 0.932 & 0.131 & 6.989 \\
 Cring strL & 6.232 & 2.920 & 0.275 & 22.319 \\
 Cring strR & 0.859 & 0.432 & 0.024 & 2.558 \\
 GIR & 29.695 & 12.721 & 1.391 & 83.960 \\
 LGSS1 & 2.055 & 1.259 & 0.042 & 8.266 \\
 LGSS2 & 6.160 & 2.973 & 0.041 & 18.499 \\
 LGSS3 & 3.057 & 1.530 & 0.077 & 10.980 \\
 LGSSc & 0.251 & 0.139 & 0.012 & 0.807 \\
 M1Baffle & 6.980 & 3.322 & 0.304 & 19.184 \\
 M1cell & 207.846 & 132.864 & 2.649 & 735.539 \\
 M1cov1 & 9.376 & 6.311 & 0.312 & 39.074 \\
 M1cov2 & 8.057 & 5.727 & 0.117 & 34.964 \\
 M1cov3 & 4.629 & 3.097 & 0.089 & 18.726 \\
 M1cov4 & 9.967 & 6.564 & 0.239 & 35.874 \\
 M1cov5 & 33.210 & 22.939 & 0.876 & 141.319 \\
 M1cov6 & 17.441 & 12.349 & 0.373 & 73.157 \\
 M1covin1 & 3.112 & 1.743 & 0.103 & 10.852 \\
 M1covin2 & 2.692 & 1.523 & 0.032 & 10.196 \\
 M1covin3 & 4.621 & 2.733 & 0.264 & 17.500 \\
 M1covin4 & 7.018 & 3.875 & 0.261 & 31.023 \\
 M1covin5 & 5.950 & 3.286 & 0.220 & 23.947 \\
 M1covin6 & 5.239 & 2.819 & 0.196 & 19.933 \\
 M1level & 22.191 & 13.213 & 0.707 & 79.724 \\
 M2Baffle & 0.897 & 0.738 & 0.003 & 8.915 \\
 M2seg1 & 0.329 & 0.216 & 0.010 & 1.666 \\
 M2seg2 & 0.314 & 0.219 & 0.007 & 2.315 \\
 M2seg3 & 0.355 & 0.314 & 0.015 & 5.512 \\
 M2seg4 & 0.391 & 0.287 & 0.024 & 4.149 \\
 M2seg5 & 0.376 & 0.260 & 0.009 & 2.024 \\
 M2seg6 & 0.380 & 0.236 & 0.005 & 1.563 \\
 M2seg7 & 0.299 & 0.216 & 0.004 & 1.395 \\
 Tbot1 & 4.385 & 2.307 & 0.136 & 14.632 \\
 Tbot2 & 7.901 & 4.440 & 0.250 & 29.391 \\
 Tbot3 & 11.227 & 6.880 & 0.507 & 43.131 \\
 Topend & 2.214 & 1.221 & 0.110 & 9.922 \\
 Tup1 & 14.702 & 9.098 & 0.557 & 61.620 \\
 Tup2 & 6.493 & 4.184 & 0.162 & 37.721 \\
 Tup3 & 7.251 & 4.205 & 0.081 & 26.193 \\
 arm1 & 1.907 & 1.367 & 0.055 & 12.375 \\
 arm2 & 1.237 & 0.965 & 0.035 & 6.321 \\
 arm3 & 2.887 & 2.002 & 0.108 & 17.945 \\
 cabletrays & 43.069 & 19.567 & 1.270 & 141.880 \\
 cabletruss & 8.300 & 4.950 & 0.333 & 33.965 \\
 platform & 65.218 & 38.956 & 1.277 & 256.683 \\
 S1 & 805.726 & 141.263 & 536.807 & 1101.536 \\
 S2 & 832.343 & 143.058 & 558.377 & 1124.133 \\
 S3 & 794.906 & 141.953 & 504.282 & 1081.705 \\
 S4 & 714.199 & 141.725 & 426.978 & 988.542 \\
 S5 & 674.199 & 142.025 & 381.385 & 938.709 \\
 S6 & 692.319 & 143.027 & 401.532 & 986.135 \\
 S7 & 663.166 & 121.381 & 442.664 & 911.644 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 191.468 & 31.813 & 111.849 & 262.015 \\
 S2 & 207.571 & 32.735 & 133.512 & 275.879 \\
 S3 & 217.469 & 32.118 & 149.353 & 291.710 \\
 S4 & 235.155 & 29.954 & 172.846 & 319.074 \\
 S5 & 245.868 & 38.008 & 163.001 & 349.274 \\
 S6 & 227.699 & 30.806 & 143.288 & 332.619 \\
 S7 & 183.230 & 25.768 & 96.850 & 258.313 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_OS7/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 371.888 & 184.699 & 17.932 & 1113.021 \\
 CringR & 117.272 & 59.737 & 2.842 & 289.308 \\
 Cring strB & 18.545 & 8.854 & 1.070 & 71.846 \\
 Cring strF & 14.351 & 7.287 & 0.750 & 52.584 \\
 Cring strL & 49.803 & 25.974 & 2.518 & 191.194 \\
 Cring strR & 5.043 & 2.405 & 0.326 & 13.631 \\
 GIR & 86.790 & 44.297 & 2.638 & 282.810 \\
 LGSS1 & 12.555 & 7.092 & 0.332 & 45.740 \\
 LGSS2 & 52.978 & 28.067 & 0.439 & 200.065 \\
 LGSS3 & 25.121 & 14.604 & 0.356 & 93.696 \\
 LGSSc & 2.339 & 1.470 & 0.037 & 9.033 \\
 M1Baffle & 27.678 & 16.775 & 0.483 & 94.652 \\
 M1cell & 791.003 & 380.775 & 44.758 & 2332.828 \\
 M1cov1 & 108.011 & 69.587 & 3.358 & 438.864 \\
 M1cov2 & 81.402 & 58.906 & 2.426 & 327.939 \\
 M1cov3 & 51.365 & 33.139 & 1.126 & 193.050 \\
 M1cov4 & 112.567 & 70.762 & 2.701 & 383.454 \\
 M1cov5 & 391.060 & 273.236 & 8.480 & 1774.059 \\
 M1cov6 & 193.378 & 132.007 & 6.261 & 760.771 \\
 M1covin1 & 19.672 & 11.026 & 0.682 & 69.750 \\
 M1covin2 & 17.385 & 10.167 & 0.667 & 62.245 \\
 M1covin3 & 28.095 & 16.629 & 0.832 & 105.569 \\
 M1covin4 & 45.107 & 25.259 & 1.205 & 178.327 \\
 M1covin5 & 41.709 & 24.637 & 0.777 & 180.702 \\
 M1covin6 & 33.537 & 18.813 & 1.068 & 116.443 \\
 M1level & 292.863 & 140.133 & 15.371 & 831.374 \\
 M2Baffle & 1.097 & 0.734 & 0.008 & 9.126 \\
 M2seg1 & 3.975 & 2.647 & 0.053 & 20.628 \\
 M2seg2 & 3.800 & 2.540 & 0.021 & 30.183 \\
 M2seg3 & 4.535 & 4.180 & 0.071 & 71.993 \\
 M2seg4 & 5.218 & 3.945 & 0.077 & 48.403 \\
 M2seg5 & 4.356 & 3.009 & 0.036 & 23.047 \\
 M2seg6 & 4.407 & 2.823 & 0.008 & 23.739 \\
 M2seg7 & 2.356 & 1.541 & 0.021 & 11.740 \\
 Tbot1 & 50.819 & 28.599 & 2.204 & 183.974 \\
 Tbot2 & 87.757 & 55.044 & 0.602 & 334.050 \\
 Tbot3 & 131.609 & 86.672 & 1.783 & 521.936 \\
 Topend & 46.048 & 28.939 & 0.213 & 224.655 \\
 Tup1 & 203.096 & 118.667 & 2.257 & 798.084 \\
 Tup2 & 105.846 & 69.561 & 1.889 & 598.927 \\
 Tup3 & 114.083 & 67.392 & 2.506 & 405.173 \\
 arm1 & 39.933 & 30.059 & 0.834 & 269.111 \\
 arm2 & 26.437 & 21.291 & 0.231 & 138.223 \\
 arm3 & 61.150 & 44.730 & 0.378 & 399.739 \\
 cabletrays & 409.078 & 192.659 & 10.660 & 1330.885 \\
 cabletruss & 122.900 & 75.710 & 4.601 & 537.520 \\
 platform & 646.654 & 302.120 & 35.976 & 1918.618 \\
 S1 & 7838.996 & 1376.460 & 5224.100 & 10714.302 \\
 S2 & 8115.287 & 1391.752 & 5436.631 & 10930.653 \\
 S3 & 7727.893 & 1380.066 & 4896.704 & 10536.368 \\
 S4 & 6921.538 & 1379.536 & 4119.552 & 9570.844 \\
 S5 & 6443.968 & 1383.437 & 3612.271 & 8987.022 \\
 S6 & 6643.214 & 1393.397 & 3739.730 & 9560.031 \\
 S7 & 95.622 & 26.684 & 16.591 & 178.064 \\
\bottomrule
\end{longtable}




\section{30 zenith - 135 azimuth - Open vents/Stowed wind screen - 7m/s}
\label{zen30az135_OS7}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/scenes/vort_tel_vort_tel_7.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 41.639 & 20.316 & 0.818 & 146.145 \\
 CringR & 14.747 & 8.016 & 0.485 & 59.539 \\
 Cring strB & 6.843 & 3.467 & 0.223 & 23.860 \\
 Cring strF & 1.933 & 0.932 & 0.131 & 6.101 \\
 Cring strL & 6.464 & 2.981 & 0.137 & 23.167 \\
 Cring strR & 0.640 & 0.298 & 0.041 & 1.862 \\
 GIR & 23.553 & 10.776 & 1.026 & 75.589 \\
 LGSS1 & 1.453 & 0.673 & 0.059 & 4.203 \\
 LGSS2 & 1.314 & 0.668 & 0.091 & 4.621 \\
 LGSS3 & 4.138 & 1.868 & 0.233 & 12.467 \\
 LGSSc & 0.804 & 0.415 & 0.036 & 3.016 \\
 M1Baffle & 1.960 & 1.141 & 0.045 & 8.766 \\
 M1cell & 138.983 & 89.052 & 4.459 & 513.490 \\
 M1cov1 & 21.346 & 15.024 & 0.238 & 114.281 \\
 M1cov2 & 4.272 & 3.212 & 0.101 & 23.576 \\
 M1cov3 & 5.354 & 3.743 & 0.181 & 21.598 \\
 M1cov4 & 3.714 & 2.532 & 0.033 & 17.317 \\
 M1cov5 & 22.068 & 16.208 & 0.392 & 104.829 \\
 M1cov6 & 32.990 & 24.326 & 0.659 & 168.466 \\
 M1covin1 & 1.090 & 0.591 & 0.087 & 3.882 \\
 M1covin2 & 1.321 & 0.733 & 0.031 & 4.379 \\
 M1covin3 & 1.180 & 0.707 & 0.034 & 4.020 \\
 M1covin4 & 0.641 & 0.477 & 0.014 & 3.181 \\
 M1covin5 & 0.903 & 0.517 & 0.042 & 3.113 \\
 M1covin6 & 0.770 & 0.462 & 0.035 & 3.157 \\
 M1level & 17.913 & 11.538 & 0.407 & 74.007 \\
 M2Baffle & 3.377 & 2.455 & 0.017 & 16.233 \\
 M2seg1 & 1.058 & 0.578 & 0.040 & 4.588 \\
 M2seg2 & 1.235 & 0.702 & 0.022 & 4.613 \\
 M2seg3 & 1.422 & 0.778 & 0.046 & 5.282 \\
 M2seg4 & 1.540 & 0.845 & 0.026 & 6.044 \\
 M2seg5 & 1.228 & 0.675 & 0.054 & 4.469 \\
 M2seg6 & 1.085 & 0.573 & 0.051 & 3.323 \\
 M2seg7 & 1.219 & 0.691 & 0.050 & 5.459 \\
 Tbot1 & 2.025 & 1.119 & 0.034 & 7.345 \\
 Tbot2 & 3.324 & 2.364 & 0.103 & 21.409 \\
 Tbot3 & 3.428 & 1.738 & 0.050 & 13.516 \\
 Topend & 5.920 & 2.786 & 0.053 & 19.272 \\
 Tup1 & 4.269 & 2.607 & 0.058 & 19.990 \\
 Tup2 & 9.909 & 5.121 & 0.156 & 30.446 \\
 Tup3 & 6.155 & 3.678 & 0.183 & 24.136 \\
 arm1 & 2.070 & 1.440 & 0.056 & 10.708 \\
 arm2 & 3.578 & 2.162 & 0.072 & 15.459 \\
 arm3 & 4.598 & 3.115 & 0.198 & 20.083 \\
 cabletrays & 40.619 & 16.380 & 1.260 & 123.722 \\
 cabletruss & 5.373 & 3.379 & 0.158 & 26.592 \\
 platform & 62.467 & 36.916 & 1.976 & 243.177 \\
 S1 & 59.387 & 14.318 & 16.545 & 101.750 \\
 S2 & 54.873 & 12.834 & 18.595 & 90.509 \\
 S3 & 45.988 & 13.759 & 11.007 & 78.950 \\
 S4 & 30.213 & 17.324 & 0.009 & 79.127 \\
 S5 & 17.799 & 12.129 & 0.011 & 68.034 \\
 S6 & 24.070 & 13.638 & 0.029 & 65.198 \\
 S7 & 24.452 & 10.295 & 0.025 & 50.097 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 86.062 & 21.040 & 20.527 & 154.753 \\
 S2 & 94.457 & 17.397 & 38.832 & 161.024 \\
 S3 & 105.401 & 18.397 & 45.458 & 170.687 \\
 S4 & 118.488 & 20.491 & 56.448 & 185.958 \\
 S5 & 137.897 & 29.884 & 35.605 & 232.814 \\
 S6 & 121.808 & 26.730 & 28.126 & 202.362 \\
 S7 & 120.975 & 21.517 & 46.663 & 198.524 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az135_OS7/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 329.746 & 183.177 & 21.142 & 1195.665 \\
 CringR & 100.634 & 52.726 & 6.687 & 352.712 \\
 Cring strB & 42.029 & 21.433 & 0.268 & 142.486 \\
 Cring strF & 14.306 & 8.130 & 0.438 & 67.105 \\
 Cring strL & 49.682 & 22.507 & 1.937 & 137.160 \\
 Cring strR & 4.562 & 2.274 & 0.223 & 19.868 \\
 GIR & 62.757 & 31.579 & 1.685 & 211.187 \\
 LGSS1 & 11.677 & 6.327 & 0.161 & 38.469 \\
 LGSS2 & 11.691 & 6.877 & 0.267 & 50.465 \\
 LGSS3 & 38.402 & 20.186 & 0.383 & 131.762 \\
 LGSSc & 6.770 & 4.282 & 0.135 & 26.615 \\
 M1Baffle & 7.737 & 5.780 & 0.118 & 43.056 \\
 M1cell & 858.241 & 429.296 & 20.976 & 2671.322 \\
 M1cov1 & 228.447 & 155.649 & 6.759 & 1232.810 \\
 M1cov2 & 47.547 & 35.430 & 0.702 & 244.771 \\
 M1cov3 & 57.171 & 40.468 & 1.477 & 224.595 \\
 M1cov4 & 42.994 & 29.656 & 1.080 & 193.952 \\
 M1cov5 & 249.727 & 176.968 & 6.552 & 1144.343 \\
 M1cov6 & 354.203 & 245.165 & 3.987 & 1733.130 \\
 M1covin1 & 6.649 & 3.671 & 0.156 & 28.016 \\
 M1covin2 & 8.593 & 5.073 & 0.210 & 31.775 \\
 M1covin3 & 8.246 & 5.218 & 0.204 & 29.733 \\
 M1covin4 & 4.083 & 3.221 & 0.037 & 21.050 \\
 M1covin5 & 5.585 & 3.285 & 0.242 & 21.726 \\
 M1covin6 & 4.751 & 2.835 & 0.070 & 20.181 \\
 M1level & 244.183 & 137.393 & 8.165 & 827.815 \\
 M2Baffle & 5.105 & 2.729 & 0.093 & 16.973 \\
 M2seg1 & 13.410 & 7.153 & 0.197 & 50.192 \\
 M2seg2 & 17.093 & 9.668 & 0.386 & 71.471 \\
 M2seg3 & 18.804 & 11.005 & 0.102 & 89.970 \\
 M2seg4 & 20.321 & 12.575 & 0.074 & 99.719 \\
 M2seg5 & 15.151 & 8.671 & 0.040 & 52.749 \\
 M2seg6 & 12.959 & 7.297 & 0.206 & 52.515 \\
 M2seg7 & 11.646 & 6.336 & 0.023 & 39.971 \\
 Tbot1 & 21.051 & 13.693 & 0.781 & 81.103 \\
 Tbot2 & 41.850 & 32.351 & 1.886 & 288.823 \\
 Tbot3 & 36.580 & 20.061 & 0.649 & 141.595 \\
 Topend & 125.481 & 65.951 & 0.991 & 455.795 \\
 Tup1 & 80.002 & 49.420 & 1.881 & 405.195 \\
 Tup2 & 158.682 & 80.282 & 4.179 & 481.365 \\
 Tup3 & 95.867 & 55.701 & 2.191 & 335.142 \\
 arm1 & 44.135 & 32.179 & 0.760 & 235.686 \\
 arm2 & 76.335 & 48.354 & 0.692 & 338.133 \\
 arm3 & 97.712 & 70.551 & 0.216 & 445.042 \\
 cabletrays & 378.322 & 178.434 & 8.270 & 1388.500 \\
 cabletruss & 88.818 & 59.698 & 3.037 & 432.899 \\
 platform & 686.548 & 387.808 & 29.743 & 2432.068 \\
 S1 & 613.919 & 146.375 & 169.026 & 1052.230 \\
 S2 & 547.936 & 127.782 & 177.792 & 910.580 \\
 S3 & 461.491 & 135.597 & 105.670 & 786.210 \\
 S4 & 495.798 & 3011.041 & 0.977 & 219121.553 \\
 S5 & 181.468 & 120.785 & 0.416 & 745.953 \\
 S6 & 222.736 & 132.188 & 0.810 & 631.717 \\
 S7 & 551.146 & 8132.007 & 0.047 & 678068.197 \\
\bottomrule
\end{longtable}




\section{30 zenith - 0 azimuth - Closed vents/Deployed wind screen - 12m/s}
\label{zen30az000_CD12}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/scenes/vort_tel_vort_tel_9.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 21.866 & 11.252 & 1.142 & 71.430 \\
 CringR & 30.741 & 19.486 & 1.216 & 120.035 \\
 Cring strB & 2.849 & 1.910 & 0.100 & 11.539 \\
 Cring strF & 3.521 & 2.114 & 0.101 & 12.469 \\
 Cring strL & 2.839 & 1.965 & 0.070 & 10.688 \\
 Cring strR & 3.714 & 2.655 & 0.066 & 15.815 \\
 GIR & 24.265 & 12.344 & 1.015 & 83.797 \\
 LGSS1 & 5.593 & 3.499 & 0.061 & 21.270 \\
 LGSS2 & 4.774 & 3.235 & 0.058 & 19.622 \\
 LGSS3 & 5.078 & 3.187 & 0.058 & 17.484 \\
 LGSSc & 1.392 & 0.994 & 0.021 & 5.828 \\
 M1Baffle & 21.235 & 14.518 & 0.968 & 82.758 \\
 M1cell & 1270.113 & 927.196 & 3.087 & 5404.538 \\
 M1cov1 & 10.044 & 6.733 & 0.161 & 39.289 \\
 M1cov2 & 8.392 & 6.790 & 0.075 & 40.630 \\
 M1cov3 & 8.786 & 6.514 & 0.037 & 40.481 \\
 M1cov4 & 4.028 & 2.679 & 0.110 & 16.115 \\
 M1cov5 & 10.364 & 7.672 & 0.099 & 45.432 \\
 M1cov6 & 7.831 & 6.182 & 0.076 & 51.726 \\
 M1covin1 & 3.125 & 1.877 & 0.086 & 12.191 \\
 M1covin2 & 3.579 & 2.236 & 0.088 & 19.216 \\
 M1covin3 & 2.873 & 1.963 & 0.062 & 12.483 \\
 M1covin4 & 1.570 & 0.998 & 0.065 & 7.638 \\
 M1covin5 & 1.853 & 1.202 & 0.067 & 7.380 \\
 M1covin6 & 2.049 & 1.279 & 0.040 & 8.677 \\
 M1level & 6.286 & 3.803 & 0.152 & 27.115 \\
 M2Baffle & 0.872 & 0.668 & 0.003 & 4.116 \\
 M2seg1 & 0.315 & 0.193 & 0.012 & 1.356 \\
 M2seg2 & 0.331 & 0.203 & 0.008 & 1.463 \\
 M2seg3 & 0.492 & 0.286 & 0.023 & 2.244 \\
 M2seg4 & 0.514 & 0.288 & 0.027 & 2.186 \\
 M2seg5 & 0.354 & 0.209 & 0.009 & 1.957 \\
 M2seg6 & 0.334 & 0.190 & 0.010 & 1.996 \\
 M2seg7 & 0.376 & 0.254 & 0.009 & 1.361 \\
 Tbot1 & 8.234 & 4.643 & 0.179 & 27.909 \\
 Tbot2 & 4.939 & 3.053 & 0.143 & 17.416 \\
 Tbot3 & 4.183 & 2.085 & 0.160 & 12.601 \\
 Topend & 3.263 & 1.596 & 0.084 & 12.854 \\
 Tup1 & 4.633 & 2.412 & 0.034 & 19.005 \\
 Tup2 & 3.460 & 1.966 & 0.101 & 13.161 \\
 Tup3 & 4.670 & 2.747 & 0.081 & 22.891 \\
 arm1 & 1.288 & 0.918 & 0.037 & 6.148 \\
 arm2 & 1.427 & 1.104 & 0.030 & 6.607 \\
 arm3 & 1.699 & 1.217 & 0.032 & 6.945 \\
 cabletrays & 84.458 & 61.319 & 1.245 & 364.083 \\
 cabletruss & 3.075 & 1.641 & 0.041 & 9.603 \\
 platform & 95.712 & 66.821 & 1.593 & 377.459 \\
 S1 & 15249.948 & 347.404 & 14229.816 & 16105.911 \\
 S2 & 15239.392 & 350.391 & 14254.796 & 16096.195 \\
 S3 & 15174.370 & 348.461 & 14124.436 & 16024.745 \\
 S4 & 15180.033 & 350.499 & 14124.451 & 16018.608 \\
 S5 & 15189.945 & 351.505 & 14107.844 & 15998.203 \\
 S6 & 15222.708 & 347.433 & 14177.493 & 16062.646 \\
 S7 & 12911.839 & 294.641 & 12025.634 & 13615.479 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 3565.159 & 81.880 & 3316.195 & 3762.270 \\
 S2 & 3570.407 & 82.167 & 3319.243 & 3761.857 \\
 S3 & 3578.219 & 81.980 & 3325.822 & 3775.060 \\
 S4 & 3589.989 & 82.685 & 3347.317 & 3794.934 \\
 S5 & 3584.606 & 83.003 & 3347.600 & 3789.740 \\
 S6 & 3571.753 & 82.245 & 3329.097 & 3776.915 \\
 S7 & 2151.036 & 62.206 & 1921.486 & 2335.345 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az000_CD12/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 199.929 & 110.304 & 6.286 & 703.955 \\
 CringR & 115.577 & 63.280 & 3.995 & 412.138 \\
 Cring strB & 21.809 & 14.972 & 0.577 & 87.986 \\
 Cring strF & 23.260 & 16.015 & 0.542 & 95.378 \\
 Cring strL & 19.519 & 13.581 & 0.362 & 76.694 \\
 Cring strR & 18.936 & 13.203 & 0.347 & 79.749 \\
 GIR & 74.103 & 38.788 & 1.378 & 245.264 \\
 LGSS1 & 53.979 & 37.916 & 0.677 & 232.915 \\
 LGSS2 & 46.117 & 33.335 & 0.203 & 182.554 \\
 LGSS3 & 46.336 & 32.865 & 0.604 & 185.403 \\
 LGSSc & 13.258 & 9.686 & 0.045 & 56.280 \\
 M1Baffle & 20.024 & 11.443 & 0.436 & 71.518 \\
 M1cell & 851.375 & 433.083 & 16.802 & 2807.188 \\
 M1cov1 & 109.494 & 73.108 & 3.980 & 458.813 \\
 M1cov2 & 92.241 & 69.945 & 1.954 & 388.575 \\
 M1cov3 & 99.854 & 71.142 & 0.962 & 459.927 \\
 M1cov4 & 45.532 & 28.861 & 0.494 & 174.965 \\
 M1cov5 & 115.142 & 81.063 & 1.951 & 480.757 \\
 M1cov6 & 84.022 & 66.263 & 1.379 & 540.916 \\
 M1covin1 & 20.055 & 11.914 & 0.424 & 73.304 \\
 M1covin2 & 24.259 & 15.127 & 0.555 & 111.589 \\
 M1covin3 & 20.109 & 14.268 & 0.162 & 91.205 \\
 M1covin4 & 10.666 & 7.229 & 0.238 & 58.215 \\
 M1covin5 & 12.060 & 8.113 & 0.153 & 53.724 \\
 M1covin6 & 13.099 & 8.459 & 0.091 & 63.035 \\
 M1level & 74.241 & 36.432 & 2.485 & 204.838 \\
 M2Baffle & 1.168 & 0.721 & 0.010 & 4.812 \\
 M2seg1 & 4.355 & 2.926 & 0.049 & 21.635 \\
 M2seg2 & 4.285 & 2.818 & 0.055 & 24.367 \\
 M2seg3 & 6.475 & 3.964 & 0.070 & 35.373 \\
 M2seg4 & 7.085 & 4.183 & 0.037 & 32.361 \\
 M2seg5 & 4.670 & 2.749 & 0.093 & 19.128 \\
 M2seg6 & 4.413 & 2.441 & 0.029 & 16.542 \\
 M2seg7 & 2.157 & 1.284 & 0.013 & 12.415 \\
 Tbot1 & 94.600 & 60.287 & 3.527 & 341.020 \\
 Tbot2 & 48.327 & 31.165 & 0.549 & 189.754 \\
 Tbot3 & 41.243 & 23.168 & 1.091 & 146.617 \\
 Topend & 58.654 & 32.388 & 0.273 & 218.726 \\
 Tup1 & 72.949 & 37.884 & 1.161 & 265.795 \\
 Tup2 & 54.277 & 31.304 & 1.022 & 191.693 \\
 Tup3 & 66.629 & 35.877 & 1.921 & 277.531 \\
 arm1 & 27.178 & 20.359 & 0.266 & 134.598 \\
 arm2 & 30.502 & 24.581 & 0.084 & 140.242 \\
 arm3 & 36.609 & 27.320 & 0.446 & 154.371 \\
 cabletrays & 193.693 & 122.474 & 5.376 & 716.669 \\
 cabletruss & 53.110 & 28.564 & 1.317 & 167.347 \\
 platform & 187.075 & 101.310 & 8.307 & 586.730 \\
 S1 & 148570.833 & 3390.467 & 138628.463 & 156921.073 \\
 S2 & 148474.636 & 3420.838 & 138823.736 & 156853.899 \\
 S3 & 147829.501 & 3398.436 & 137622.018 & 156163.964 \\
 S4 & 147912.599 & 3418.896 & 137632.059 & 156097.041 \\
 S5 & 147997.203 & 3427.495 & 137430.964 & 155857.530 \\
 S6 & 148300.669 & 3383.394 & 138124.380 & 156481.511 \\
 S7 & 1681.475 & 48.600 & 1519.242 & 1798.100 \\
\bottomrule
\end{longtable}




\section{30 zenith - 45 azimuth - Closed vents/Deployed wind screen - 12m/s}
\label{zen30az045_CD12}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/scenes/vort_tel_vort_tel_9.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 16.599 & 8.812 & 0.641 & 54.174 \\
 CringR & 19.661 & 11.109 & 0.712 & 70.150 \\
 Cring strB & 2.533 & 1.187 & 0.074 & 7.537 \\
 Cring strF & 1.458 & 0.724 & 0.074 & 4.970 \\
 Cring strL & 0.637 & 0.315 & 0.024 & 2.505 \\
 Cring strR & 1.045 & 0.525 & 0.053 & 3.494 \\
 GIR & 19.778 & 9.043 & 1.210 & 60.607 \\
 LGSS1 & 2.671 & 1.575 & 0.114 & 13.140 \\
 LGSS2 & 1.990 & 1.022 & 0.148 & 10.772 \\
 LGSS3 & 1.049 & 0.517 & 0.046 & 3.670 \\
 LGSSc & 0.676 & 0.314 & 0.055 & 2.274 \\
 M1Baffle & 7.551 & 3.784 & 0.484 & 23.216 \\
 M1cell & 200.601 & 132.015 & 4.486 & 820.178 \\
 M1cov1 & 8.409 & 5.942 & 0.184 & 34.493 \\
 M1cov2 & 6.247 & 4.398 & 0.208 & 27.690 \\
 M1cov3 & 7.282 & 5.029 & 0.158 & 26.171 \\
 M1cov4 & 6.310 & 4.264 & 0.248 & 27.291 \\
 M1cov5 & 10.955 & 7.524 & 0.162 & 38.269 \\
 M1cov6 & 6.975 & 4.724 & 0.145 & 24.766 \\
 M1covin1 & 2.007 & 1.102 & 0.133 & 7.662 \\
 M1covin2 & 2.364 & 1.432 & 0.091 & 9.911 \\
 M1covin3 & 2.784 & 1.495 & 0.136 & 10.749 \\
 M1covin4 & 1.856 & 1.111 & 0.062 & 7.780 \\
 M1covin5 & 1.968 & 1.144 & 0.014 & 7.699 \\
 M1covin6 & 1.731 & 1.041 & 0.028 & 8.018 \\
 M1level & 8.079 & 4.898 & 0.373 & 36.906 \\
 M2Baffle & 0.715 & 0.573 & 0.006 & 3.699 \\
 M2seg1 & 0.280 & 0.167 & 0.021 & 1.341 \\
 M2seg2 & 0.283 & 0.188 & 0.006 & 1.519 \\
 M2seg3 & 0.255 & 0.160 & 0.011 & 1.087 \\
 M2seg4 & 0.216 & 0.133 & 0.010 & 0.924 \\
 M2seg5 & 0.195 & 0.122 & 0.007 & 1.074 \\
 M2seg6 & 0.228 & 0.126 & 0.013 & 0.998 \\
 M2seg7 & 0.224 & 0.146 & 0.010 & 1.032 \\
 Tbot1 & 4.595 & 2.914 & 0.144 & 22.679 \\
 Tbot2 & 5.204 & 3.042 & 0.159 & 19.550 \\
 Tbot3 & 2.858 & 1.695 & 0.121 & 10.892 \\
 Topend & 1.320 & 0.692 & 0.079 & 8.836 \\
 Tup1 & 3.708 & 2.682 & 0.145 & 20.217 \\
 Tup2 & 3.071 & 2.061 & 0.120 & 14.541 \\
 Tup3 & 1.500 & 0.899 & 0.029 & 6.716 \\
 arm1 & 0.544 & 0.444 & 0.027 & 4.345 \\
 arm2 & 1.257 & 1.028 & 0.037 & 10.139 \\
 arm3 & 0.463 & 0.436 & 0.014 & 4.990 \\
 cabletrays & 20.558 & 10.421 & 0.688 & 64.759 \\
 cabletruss & 1.658 & 1.128 & 0.034 & 8.505 \\
 platform & 35.240 & 23.799 & 0.719 & 145.255 \\
 S1 & 2264.895 & 268.157 & 1733.117 & 2745.351 \\
 S2 & 2263.719 & 269.930 & 1722.706 & 2744.414 \\
 S3 & 2237.674 & 269.758 & 1688.534 & 2739.262 \\
 S4 & 2228.197 & 269.369 & 1698.506 & 2689.188 \\
 S5 & 2256.516 & 266.132 & 1717.149 & 2745.829 \\
 S6 & 2271.569 & 271.799 & 1723.653 & 2782.559 \\
 S7 & 1906.902 & 227.927 & 1454.829 & 2322.292 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 529.789 & 60.259 & 409.019 & 642.332 \\
 S2 & 539.356 & 61.519 & 410.167 & 643.869 \\
 S3 & 537.116 & 62.801 & 402.906 & 650.368 \\
 S4 & 530.876 & 63.063 & 399.049 & 644.792 \\
 S5 & 529.947 & 60.540 & 401.879 & 651.116 \\
 S6 & 528.658 & 61.604 & 400.641 & 659.624 \\
 S7 & 227.555 & 49.053 & 81.648 & 351.438 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az045_CD12/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 120.666 & 66.024 & 1.117 & 374.265 \\
 CringR & 139.716 & 82.978 & 5.640 & 512.842 \\
 Cring strB & 16.575 & 8.133 & 0.756 & 51.319 \\
 Cring strF & 9.069 & 4.943 & 0.191 & 32.491 \\
 Cring strL & 4.889 & 2.530 & 0.038 & 14.572 \\
 Cring strR & 6.764 & 3.247 & 0.277 & 21.562 \\
 GIR & 59.451 & 31.388 & 2.173 & 226.634 \\
 LGSS1 & 22.316 & 12.561 & 0.406 & 108.562 \\
 LGSS2 & 17.110 & 9.254 & 0.479 & 55.241 \\
 LGSS3 & 9.542 & 5.417 & 0.130 & 38.395 \\
 LGSSc & 6.711 & 3.655 & 0.040 & 22.227 \\
 M1Baffle & 31.818 & 18.181 & 0.267 & 113.147 \\
 M1cell & 599.748 & 330.283 & 26.202 & 2140.025 \\
 M1cov1 & 94.209 & 65.506 & 2.993 & 398.212 \\
 M1cov2 & 73.333 & 49.784 & 1.179 & 292.962 \\
 M1cov3 & 80.743 & 54.429 & 2.123 & 277.766 \\
 M1cov4 & 72.131 & 48.222 & 1.764 & 271.172 \\
 M1cov5 & 122.885 & 81.032 & 2.422 & 420.425 \\
 M1cov6 & 78.509 & 50.578 & 1.248 & 292.797 \\
 M1covin1 & 13.183 & 7.482 & 0.370 & 50.217 \\
 M1covin2 & 14.933 & 9.090 & 0.355 & 64.212 \\
 M1covin3 & 18.595 & 10.459 & 0.627 & 65.521 \\
 M1covin4 & 12.890 & 8.292 & 0.168 & 59.791 \\
 M1covin5 & 13.426 & 8.288 & 0.151 & 57.969 \\
 M1covin6 & 11.164 & 7.084 & 0.259 & 52.714 \\
 M1level & 108.963 & 53.656 & 5.348 & 514.212 \\
 M2Baffle & 0.834 & 0.568 & 0.011 & 4.068 \\
 M2seg1 & 3.522 & 2.390 & 0.073 & 23.349 \\
 M2seg2 & 3.507 & 2.719 & 0.007 & 26.199 \\
 M2seg3 & 2.820 & 1.838 & 0.028 & 13.521 \\
 M2seg4 & 2.278 & 1.335 & 0.006 & 11.806 \\
 M2seg5 & 2.158 & 1.277 & 0.026 & 10.532 \\
 M2seg6 & 2.846 & 1.790 & 0.026 & 13.706 \\
 M2seg7 & 1.782 & 1.109 & 0.016 & 9.946 \\
 Tbot1 & 52.153 & 37.567 & 0.851 & 293.914 \\
 Tbot2 & 55.267 & 33.971 & 1.017 & 213.494 \\
 Tbot3 & 32.333 & 21.475 & 1.505 & 135.254 \\
 Topend & 27.064 & 16.934 & 0.373 & 212.129 \\
 Tup1 & 52.499 & 36.306 & 1.389 & 249.240 \\
 Tup2 & 44.213 & 28.220 & 0.818 & 201.186 \\
 Tup3 & 21.290 & 12.262 & 0.436 & 79.451 \\
 arm1 & 11.486 & 9.838 & 0.226 & 95.254 \\
 arm2 & 26.879 & 22.855 & 0.488 & 221.714 \\
 arm3 & 9.787 & 9.683 & 0.071 & 110.088 \\
 cabletrays & 120.701 & 53.363 & 4.278 & 323.588 \\
 cabletruss & 23.340 & 16.555 & 0.699 & 126.286 \\
 platform & 381.754 & 244.763 & 9.006 & 1509.135 \\
 S1 & 22059.291 & 2612.975 & 16872.345 & 26751.341 \\
 S2 & 22087.422 & 2643.500 & 16795.048 & 26802.286 \\
 S3 & 21787.394 & 2630.779 & 16425.472 & 26707.010 \\
 S4 & 21693.890 & 2625.768 & 16526.728 & 26214.570 \\
 S5 & 22002.495 & 2597.735 & 16748.959 & 26810.850 \\
 S6 & 22133.789 & 2647.412 & 16801.971 & 27110.904 \\
 S7 & 110.336 & 20.499 & 41.978 & 169.254 \\
\bottomrule
\end{longtable}




\section{30 zenith - 90 azimuth - Closed vents/Deployed wind screen - 12m/s}
\label{zen30az090_CD12}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/scenes/vort_tel_vort_tel_9.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 16.808 & 8.371 & 0.932 & 49.393 \\
 CringR & 41.292 & 24.244 & 1.699 & 158.615 \\
 Cring strB & 2.760 & 1.336 & 0.068 & 8.978 \\
 Cring strF & 2.578 & 1.228 & 0.128 & 8.592 \\
 Cring strL & 0.946 & 0.443 & 0.041 & 3.820 \\
 Cring strR & 2.066 & 0.947 & 0.055 & 6.020 \\
 GIR & 26.886 & 12.152 & 0.921 & 80.047 \\
 LGSS1 & 3.578 & 2.437 & 0.071 & 20.887 \\
 LGSS2 & 1.634 & 0.918 & 0.121 & 7.027 \\
 LGSS3 & 0.976 & 0.566 & 0.031 & 3.668 \\
 LGSSc & 0.694 & 0.324 & 0.038 & 2.625 \\
 M1Baffle & 4.300 & 2.133 & 0.349 & 16.565 \\
 M1cell & 163.579 & 101.094 & 5.279 & 713.427 \\
 M1cov1 & 2.882 & 2.066 & 0.041 & 12.045 \\
 M1cov2 & 11.719 & 10.439 & 0.306 & 68.252 \\
 M1cov3 & 18.630 & 15.025 & 0.245 & 91.712 \\
 M1cov4 & 8.710 & 6.902 & 0.139 & 41.360 \\
 M1cov5 & 4.303 & 3.257 & 0.027 & 16.906 \\
 M1cov6 & 7.581 & 5.404 & 0.213 & 34.750 \\
 M1covin1 & 1.165 & 0.724 & 0.047 & 4.520 \\
 M1covin2 & 1.488 & 0.809 & 0.044 & 5.089 \\
 M1covin3 & 2.443 & 1.398 & 0.027 & 8.485 \\
 M1covin4 & 2.085 & 1.230 & 0.051 & 10.030 \\
 M1covin5 & 1.372 & 0.910 & 0.062 & 5.998 \\
 M1covin6 & 1.217 & 0.669 & 0.059 & 4.919 \\
 M1level & 12.624 & 8.669 & 0.384 & 51.620 \\
 M2Baffle & 0.915 & 0.905 & 0.005 & 8.665 \\
 M2seg1 & 0.240 & 0.186 & 0.013 & 1.404 \\
 M2seg2 & 0.269 & 0.209 & 0.005 & 1.291 \\
 M2seg3 & 0.277 & 0.220 & 0.013 & 1.444 \\
 M2seg4 & 0.288 & 0.243 & 0.006 & 2.238 \\
 M2seg5 & 0.316 & 0.316 & 0.007 & 3.296 \\
 M2seg6 & 0.268 & 0.259 & 0.004 & 3.492 \\
 M2seg7 & 0.249 & 0.220 & 0.006 & 1.883 \\
 Tbot1 & 2.148 & 1.218 & 0.056 & 7.616 \\
 Tbot2 & 3.717 & 2.303 & 0.158 & 16.773 \\
 Tbot3 & 2.795 & 1.563 & 0.091 & 9.234 \\
 Topend & 1.822 & 1.715 & 0.167 & 15.170 \\
 Tup1 & 1.548 & 1.278 & 0.022 & 10.013 \\
 Tup2 & 1.419 & 1.084 & 0.031 & 6.377 \\
 Tup3 & 2.059 & 1.249 & 0.065 & 6.919 \\
 arm1 & 0.463 & 0.592 & 0.010 & 8.412 \\
 arm2 & 0.468 & 0.518 & 0.012 & 6.357 \\
 arm3 & 0.832 & 0.677 & 0.015 & 5.019 \\
 cabletrays & 21.199 & 9.929 & 0.542 & 72.777 \\
 cabletruss & 2.150 & 1.421 & 0.052 & 8.328 \\
 platform & 34.176 & 20.246 & 1.580 & 113.172 \\
 S1 & 854.826 & 18.621 & 790.977 & 904.184 \\
 S2 & 866.639 & 23.279 & 787.273 & 923.018 \\
 S3 & 855.938 & 22.001 & 785.259 & 921.119 \\
 S4 & 836.535 & 17.597 & 773.485 & 892.589 \\
 S5 & 827.098 & 15.919 & 772.519 & 871.138 \\
 S6 & 844.012 & 16.436 & 793.002 & 884.833 \\
 S7 & 732.667 & 12.418 & 690.912 & 763.233 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 203.771 & 9.327 & 177.804 & 245.976 \\
 S2 & 218.402 & 12.754 & 187.308 & 267.575 \\
 S3 & 223.936 & 12.773 & 194.346 & 273.058 \\
 S4 & 218.225 & 9.291 & 193.470 & 268.721 \\
 S5 & 206.486 & 7.215 & 186.130 & 245.295 \\
 S6 & 202.722 & 8.340 & 178.943 & 241.223 \\
 S7 & 33.892 & 17.232 & 1.028 & 106.027 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az090_CD12/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 109.033 & 54.356 & 3.160 & 375.382 \\
 CringR & 284.646 & 154.886 & 8.965 & 1191.295 \\
 Cring strB & 17.483 & 9.369 & 0.389 & 61.452 \\
 Cring strF & 17.363 & 8.552 & 0.757 & 53.691 \\
 Cring strL & 6.839 & 3.451 & 0.140 & 24.491 \\
 Cring strR & 14.642 & 7.756 & 0.254 & 50.587 \\
 GIR & 90.083 & 50.137 & 5.734 & 322.410 \\
 LGSS1 & 25.081 & 15.906 & 0.230 & 125.753 \\
 LGSS2 & 12.928 & 7.326 & 0.105 & 51.031 \\
 LGSS3 & 6.637 & 3.873 & 0.149 & 27.226 \\
 LGSSc & 5.187 & 2.674 & 0.067 & 16.594 \\
 M1Baffle & 19.538 & 10.357 & 0.471 & 81.154 \\
 M1cell & 730.738 & 380.870 & 21.391 & 2155.649 \\
 M1cov1 & 33.685 & 23.505 & 0.717 & 135.675 \\
 M1cov2 & 130.909 & 116.698 & 1.843 & 760.331 \\
 M1cov3 & 208.166 & 166.792 & 2.208 & 1015.187 \\
 M1cov4 & 96.708 & 75.360 & 1.568 & 483.327 \\
 M1cov5 & 48.036 & 35.328 & 0.649 & 198.313 \\
 M1cov6 & 86.266 & 58.632 & 2.173 & 407.815 \\
 M1covin1 & 7.510 & 4.999 & 0.190 & 32.517 \\
 M1covin2 & 9.788 & 5.725 & 0.117 & 35.038 \\
 M1covin3 & 16.696 & 9.728 & 0.199 & 59.461 \\
 M1covin4 & 12.919 & 7.768 & 0.137 & 59.768 \\
 M1covin5 & 8.923 & 5.828 & 0.230 & 37.288 \\
 M1covin6 & 7.648 & 4.064 & 0.064 & 28.812 \\
 M1level & 156.414 & 105.682 & 2.100 & 719.112 \\
 M2Baffle & 0.827 & 0.675 & 0.021 & 10.392 \\
 M2seg1 & 2.659 & 1.948 & 0.017 & 17.786 \\
 M2seg2 & 2.924 & 2.090 & 0.017 & 16.045 \\
 M2seg3 & 2.871 & 2.172 & 0.020 & 15.221 \\
 M2seg4 & 3.035 & 2.477 & 0.056 & 17.805 \\
 M2seg5 & 3.503 & 3.259 & 0.016 & 32.357 \\
 M2seg6 & 2.996 & 2.556 & 0.059 & 25.443 \\
 M2seg7 & 1.681 & 1.188 & 0.018 & 9.443 \\
 Tbot1 & 21.070 & 14.226 & 0.444 & 78.927 \\
 Tbot2 & 41.833 & 28.682 & 0.791 & 197.050 \\
 Tbot3 & 28.694 & 17.418 & 0.743 & 113.828 \\
 Topend & 36.296 & 33.917 & 0.653 & 303.113 \\
 Tup1 & 23.642 & 19.170 & 0.551 & 182.580 \\
 Tup2 & 21.125 & 15.325 & 0.443 & 86.506 \\
 Tup3 & 30.855 & 18.888 & 0.440 & 108.578 \\
 arm1 & 9.795 & 12.876 & 0.090 & 184.403 \\
 arm2 & 9.974 & 11.360 & 0.030 & 140.630 \\
 arm3 & 17.956 & 15.078 & 0.255 & 110.928 \\
 cabletrays & 152.301 & 72.345 & 7.056 & 424.040 \\
 cabletruss & 33.393 & 21.909 & 1.016 & 127.762 \\
 platform & 291.920 & 147.122 & 7.509 & 889.188 \\
 S1 & 8327.541 & 183.305 & 7692.686 & 8814.148 \\
 S2 & 8443.872 & 230.861 & 7660.005 & 9021.129 \\
 S3 & 8310.369 & 220.420 & 7601.651 & 8952.554 \\
 S4 & 8146.775 & 179.253 & 7533.115 & 8694.793 \\
 S5 & 8049.096 & 157.779 & 7511.511 & 8479.337 \\
 S6 & 8230.742 & 162.782 & 7722.130 & 8651.039 \\
 S7 & 73.765 & 10.895 & 44.224 & 123.025 \\
\bottomrule
\end{longtable}




\section{30 zenith - 180 azimuth - Closed vents/Deployed wind screen - 12m/s}
\label{zen30az180_CD12}

\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/scenes/vort_tel_vort_tel_9.000000e+02"}}}

\subsection{Forces [N]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 20.198 & 12.007 & 0.889 & 79.907 \\
 CringR & 23.446 & 12.555 & 0.711 & 66.854 \\
 Cring strB & 2.307 & 1.248 & 0.071 & 7.116 \\
 Cring strF & 1.685 & 0.933 & 0.063 & 5.587 \\
 Cring strL & 0.652 & 0.403 & 0.009 & 2.492 \\
 Cring strR & 1.002 & 0.583 & 0.046 & 4.128 \\
 GIR & 23.671 & 10.826 & 0.174 & 66.095 \\
 LGSS1 & 4.966 & 2.952 & 0.582 & 26.198 \\
 LGSS2 & 2.075 & 1.363 & 0.072 & 9.298 \\
 LGSS3 & 4.776 & 3.098 & 0.038 & 21.484 \\
 LGSSc & 0.667 & 0.401 & 0.031 & 3.241 \\
 M1Baffle & 9.779 & 5.395 & 0.886 & 41.909 \\
 M1cell & 290.257 & 213.179 & 7.047 & 1256.871 \\
 M1cov1 & 18.090 & 13.153 & 0.254 & 91.538 \\
 M1cov2 & 27.466 & 21.540 & 0.149 & 144.474 \\
 M1cov3 & 10.597 & 11.522 & 0.150 & 85.139 \\
 M1cov4 & 3.525 & 3.617 & 0.063 & 33.575 \\
 M1cov5 & 4.213 & 3.178 & 0.070 & 22.350 \\
 M1cov6 & 12.487 & 11.409 & 0.225 & 96.192 \\
 M1covin1 & 4.553 & 3.137 & 0.111 & 19.496 \\
 M1covin2 & 3.219 & 2.398 & 0.045 & 16.647 \\
 M1covin3 & 3.805 & 3.203 & 0.193 & 24.532 \\
 M1covin4 & 3.326 & 2.094 & 0.119 & 14.643 \\
 M1covin5 & 3.254 & 2.371 & 0.052 & 14.512 \\
 M1covin6 & 4.460 & 3.207 & 0.068 & 19.163 \\
 M1level & 11.534 & 8.842 & 0.303 & 72.767 \\
 M2Baffle & 4.408 & 3.305 & 0.025 & 23.626 \\
 M2seg1 & 2.988 & 1.794 & 0.117 & 12.367 \\
 M2seg2 & 2.708 & 1.574 & 0.144 & 12.919 \\
 M2seg3 & 1.727 & 0.976 & 0.036 & 7.173 \\
 M2seg4 & 1.516 & 0.839 & 0.027 & 5.662 \\
 M2seg5 & 1.784 & 1.014 & 0.059 & 8.372 \\
 M2seg6 & 2.196 & 1.270 & 0.093 & 10.045 \\
 M2seg7 & 1.830 & 1.216 & 0.036 & 7.816 \\
 Tbot1 & 5.033 & 2.754 & 0.189 & 18.298 \\
 Tbot2 & 3.080 & 1.816 & 0.061 & 10.426 \\
 Tbot3 & 7.857 & 4.846 & 0.313 & 25.890 \\
 Topend & 23.553 & 10.397 & 1.680 & 70.918 \\
 Tup1 & 12.804 & 6.590 & 0.517 & 47.910 \\
 Tup2 & 10.951 & 6.478 & 0.237 & 46.023 \\
 Tup3 & 8.395 & 4.573 & 0.410 & 34.188 \\
 arm1 & 9.935 & 7.031 & 0.207 & 61.246 \\
 arm2 & 8.222 & 6.356 & 0.305 & 60.976 \\
 arm3 & 5.497 & 4.254 & 0.056 & 33.518 \\
 cabletrays & 25.517 & 14.704 & 0.824 & 89.477 \\
 cabletruss & 6.462 & 3.709 & 0.162 & 25.346 \\
 platform & 25.961 & 15.143 & 0.138 & 97.180 \\
 S1 & 918.721 & 71.491 & 672.391 & 1062.066 \\
 S2 & 899.969 & 73.141 & 636.690 & 1080.257 \\
 S3 & 955.915 & 72.773 & 619.409 & 1105.790 \\
 S4 & 982.702 & 71.040 & 764.889 & 1138.583 \\
 S5 & 986.667 & 71.110 & 794.081 & 1142.546 \\
 S6 & 964.986 & 82.289 & 750.884 & 1128.936 \\
 S7 & 792.362 & 53.755 & 657.135 & 918.182 \\
\bottomrule
\end{longtable}

\subsubsection{M1 segment net forces}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 S1 & 236.382 & 24.297 & 164.831 & 352.204 \\
 S2 & 248.082 & 35.663 & 178.264 & 388.025 \\
 S3 & 239.184 & 20.007 & 185.377 & 333.764 \\
 S4 & 238.169 & 18.909 & 190.158 & 295.148 \\
 S5 & 235.560 & 18.681 & 183.044 & 288.594 \\
 S6 & 234.584 & 22.733 & 174.042 & 385.281 \\
 S7 & 187.264 & 67.411 & 11.920 & 434.170 \\
\bottomrule
\end{longtable}

\subsubsection{C-Rings}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/c-ring_parts-detrend"}}}
\subsubsection{M1 Cell}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m1-cell-detrend"}}}
\subsubsection{M1 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m1-segments"}}}
\subsubsection{Lower trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/lower-truss-detrend"}}}
\subsubsection{Upper trusses}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/upper-truss-detrend"}}}
\subsubsection{Top-end}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/top-end-detrend"}}}
\subsubsection{M2 segments}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m2-segments-detrend"}}}
\subsubsection{M1 \& M2 baffles}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m12-baffles-detrend"}}}
\subsubsection{M1 outer covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m1-outer-covers-detrend"}}}
\subsubsection{M1 inner covers}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/m1-inner-covers-detrend"}}}
\subsubsection{GIR}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/gir-detrend"}}}
\subsubsection{Prime focus assembly arms}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/pfa-arms-detrend"}}}
\subsubsection{Laser launch assemblies}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/lgs-detrend"}}}
\subsubsection{Platforms \& cable wraps}
\includegraphics[width=0.8\textwidth]{{{"/fsx/Baseline2021/Baseline2021/Baseline2021/CASES/zen30az180_CD12/platforms-cables-detrend"}}}

\subsection{Moments [N.M]}
\begin{longtable}{crrrr}\toprule
 ELEMENT & MEAN & STD & MIN & MAX \\\hline
 CringL & 153.494 & 88.614 & 5.043 & 543.891 \\
 CringR & 122.066 & 67.414 & 2.463 & 387.716 \\
 Cring strB & 13.647 & 7.921 & 0.453 & 53.557 \\
 Cring strF & 13.223 & 7.906 & 0.332 & 46.387 \\
 Cring strL & 4.293 & 2.771 & 0.085 & 15.394 \\
 Cring strR & 4.804 & 2.842 & 0.111 & 16.666 \\
 GIR & 73.225 & 39.634 & 1.697 & 222.119 \\
 LGSS1 & 36.367 & 26.584 & 0.494 & 181.860 \\
 LGSS2 & 11.500 & 6.819 & 0.081 & 42.297 \\
 LGSS3 & 21.821 & 15.883 & 0.395 & 105.873 \\
 LGSSc & 6.575 & 4.595 & 0.073 & 29.673 \\
 M1Baffle & 37.287 & 24.384 & 0.157 & 172.296 \\
 M1cell & 722.099 & 370.447 & 15.234 & 1995.212 \\
 M1cov1 & 196.725 & 139.456 & 3.442 & 993.766 \\
 M1cov2 & 297.206 & 231.881 & 4.000 & 1557.235 \\
 M1cov3 & 113.255 & 123.202 & 2.727 & 1022.328 \\
 M1cov4 & 39.753 & 38.055 & 0.328 & 346.270 \\
 M1cov5 & 46.961 & 35.258 & 1.109 & 270.185 \\
 M1cov6 & 136.806 & 125.332 & 1.518 & 999.068 \\
 M1covin1 & 30.278 & 21.275 & 1.175 & 141.137 \\
 M1covin2 & 20.721 & 15.434 & 0.690 & 117.633 \\
 M1covin3 & 25.253 & 22.814 & 0.365 & 176.348 \\
 M1covin4 & 21.108 & 13.867 & 0.395 & 102.687 \\
 M1covin5 & 19.679 & 14.398 & 0.251 & 90.550 \\
 M1covin6 & 29.005 & 21.331 & 0.398 & 115.131 \\
 M1level & 172.078 & 136.202 & 4.067 & 1108.804 \\
 M2Baffle & 6.313 & 3.521 & 0.043 & 29.565 \\
 M2seg1 & 33.537 & 21.777 & 0.300 & 150.956 \\
 M2seg2 & 29.972 & 17.203 & 0.477 & 149.250 \\
 M2seg3 & 21.672 & 14.308 & 0.042 & 106.508 \\
 M2seg4 & 21.182 & 13.764 & 0.186 & 116.907 \\
 M2seg5 & 21.515 & 13.454 & 0.344 & 99.194 \\
 M2seg6 & 24.665 & 15.365 & 0.092 & 107.344 \\
 M2seg7 & 10.673 & 7.217 & 0.083 & 45.749 \\
 Tbot1 & 51.872 & 30.602 & 3.549 & 209.597 \\
 Tbot2 & 31.787 & 22.085 & 0.725 & 146.206 \\
 Tbot3 & 86.775 & 59.678 & 2.081 & 296.142 \\
 Topend & 432.369 & 231.338 & 4.624 & 1496.795 \\
 Tup1 & 211.665 & 118.619 & 4.511 & 960.736 \\
 Tup2 & 193.344 & 124.988 & 5.559 & 902.465 \\
 Tup3 & 132.739 & 67.638 & 0.825 & 492.741 \\
 arm1 & 213.314 & 159.164 & 2.343 & 1355.976 \\
 arm2 & 174.515 & 142.203 & 1.273 & 1349.662 \\
 arm3 & 116.557 & 95.317 & 1.714 & 734.741 \\
 cabletrays & 119.638 & 62.092 & 5.176 & 377.909 \\
 cabletruss & 115.076 & 65.222 & 2.887 & 443.861 \\
 platform & 245.874 & 160.242 & 4.438 & 936.362 \\
 S1 & 8995.796 & 706.901 & 6457.119 & 10431.835 \\
 S2 & 8787.108 & 733.231 & 6086.055 & 10602.758 \\
 S3 & 9355.098 & 721.272 & 6154.097 & 10843.113 \\
 S4 & 9596.802 & 696.836 & 7459.286 & 11121.607 \\
 S5 & 9629.199 & 693.092 & 7730.157 & 11171.785 \\
 S6 & 9437.954 & 805.066 & 7406.213 & 11040.829 \\
 S7 & 188.483 & 48.386 & 37.483 & 420.016 \\
\bottomrule
\end{longtable}



